**MultiSpeak Version 4.1.6**

**Revision History**

**Build V4.1.6 Release – Issued 08/31/2012.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd schema into the WSDL. Further investigation of this issue is on-going.

**UML and schema changes**:

1. Added the existing gpsLocation object to the assessmentLocation.
2. Added the existing photo object to the assessmentLocation object.
3. Added an expiresOn element (of type mspDateTime) to assessment object.
4. Added outageReasonItem.categoryGroup of type xs:string.
5. Added existing electricLocationFields to the end of transformerBank object
6. Added a new surgeArrestor object
7. Added array of new surgeArrestor object to physicalObjectList and spatialFeatureGroup
8. Added XSD Stereotypes to:
   * CDState.timestamp
   * CDEnabledItem.meterID
   * CDStateChange.timestamp
   * All DRProgram elements
   * All DRProgramEnrollment elements
   * All configurationStatusItem elements
   * Content.fileName, Content.sourceFilePath, Content.attachDateTime, Content.caption
   * domainMemberChange.description
   * electricMeter.meterBaseID, electricMeter.meterConnectionStatus
   * electricService.rateCode
   * errorStringList.errorString
   * gasMeter.meterConnectionStatus
   * gasMeterExchange.timestamp
   * gaseService.rateCode
   * informationList.informationItem
   * All meterConfigurationStatus elements
   * mspMeter.meterStatusList
   * otherMeter.meterConnectionStatus.
   * otherMeterExchange.timestamp
   * otherService.rateCode
   * outageEventStatus.outageAttachments
   * propaneMeter.meterConnectionStatus
   * propaneMeterExchange.timestamp
   * propaneService.rateCode
   * readingValue.fieldName, readingValue.readingStatusCode, readingValue.readingTypeCode
   * All thresholdMonitoringItem elements
   * All thresholdNotificationItem elements
   * waterMeter.meterConnectionStatus
   * waterMeterExchange.timestamp
   * otherService.rateCode
9. Added contactInfo object to end of serviceLocation as an optional element. Marked existing serviceLocation.phoneList and serviceLocation.serviceAddress as deprecated.
10. Added annotation on the DRProgram.DRProgramStatus element.
11. Deprecated the loadManagementEvent.groupName.
12. Added an optional configuredReadingTypes at the end of the electricMeter, gasMeter, waterMeter, propaneMeter, otherMeter.
13. Added locationAssociations to the end of the workOrder object.
14. Added workHistoryEvents to the end of the workOrder.
15. Added new serviceOrderNumbers to end of the workOrder object.
16. Added a new optional gridLocation element (of type gridLocation) to the end of the workOrder object.
17. Added new enumeration capacitorSwitchStatus with the list of: [Connected | Disconnected | InTransition | Failed | Other | Unknown]
18. Added new capacitorBankSwitch and capacitorBankSwitches
19. Added AMRVendor, AMRDeviceType and meterID to the end of CDDevice.
20. Added existing new string-type meterCommAddress to the end of the electricMeter, gasMeter, waterMeter, propaneMeter and otherMeter
21. Added new billingTerms on the end of connectDisconnectEvent.
22. Added a new object billingStatusInformation to the existing electricService, gasService, waterService, propaneService and otherService objects
23. Added new remoteReconnectSetting enum and added to electricMeter, waterMeter, gasMeter, propaneMeter and otherMeter.
24. Added alternateContactList and added to the customer object.
25. Added new loadManagementDeviceRelay and loadManagementDeviceRelays elements.
26. Added loadManagementDeviceRelays, AMRDeviceType, AMRVendor, and utilityInfo to the end loadManagementDevice.
27. Added otherQualityCode to the end of the scadaAnalog and scadaStatus objects.
28. Added serviceSubType element on the end of the electricService, gasService, waterService, propaneService, otherService.
29. Changed demandResponseEvent.randomizeEventStart and demandResponseEvent.randomizeEventEnd to be optional.
30. Added new enumeration IHDMessageType with the enumeration values of [Other | BillingMessage | Message | Unknown].
31. loadManagementEvent.substationName, loadManagementEvent.feederName, loadManagementEvent.feederNumber marked as deprecated and to be removed in v5.0
32. Added new enumeration DRProgramEnrollmentStatus with values of [ Other | Active | Inactive | Pending | Unknown]
33. Added new elements DRProgramEnrollmentStatus (of type DRProgramEnrollmentStatus) and otherDRProgramEnrollmentStatus (of type xs:string) to the end of the DRProgramEnrollment object.
34. Fixed annotation on electricLocationFields.phaseCode to read “Phasing code for this electric service”

**Web Service Method Changes**:

1. Added responseURL (of type string) to all instances of InitiateDemandResponseSetup.
2. Added a new GetMetersByMeterConnectionStatus on CB\_Server and MDM\_Server.
3. Deprecated the InitiateHANRegistrationStatus object. Created new registrationStatus object and changed the payload of the InitiateHANRegistrationStatusRequest method to use the new registrationStatus object.
4. Added transactionID at the end of the calling parameter list of ThermostatAddNotification and ThermostatRemoveNotification.
5. Added GetOutageEventsByDate to OA\_Server
6. Added SurgeArrestorChangedNotification to the CB\_Server, GIS\_Server, NOT\_Server.
7. Added UpdateOutageETOR to OA\_Server.
8. Added GetAllActiveNonOutageCalls to OA\_Server.
9. Added AssignCrewsToAssessment and UnassignCrewsFromAssessment to OA\_Server.
10. Added GetCapBankSwitchStatusesBySwitchIDs to DR\_Server.
11. Added PowerFactorManagementEventNotification on SCADA\_Server, EA\_Server, NOT\_Server.
12. Added transactionID and responseURL calling parameters on InitiatePowerFactorManagementEvent, InitiateLoadManagementEvent, InitiateLoadManagementEvents on MDM\_Server and DR\_Server.
13. Added MeterChangedNotification on DR\_Server.
14. Added responseURL on DR\_Server and MDM\_Server to the following methods:

InitiateDemandResponseEventStatusRequestToGroup  
InitiateDemandResponseEventStatusRequest  
InitiateDemandResponseEvent  
InitiateDemandResponseEventToGroup  
CancelDemandResponseEvent  
CancelDemandResponseEventToGroup  
InitiateDemandResponseSetup  
InitiateCriticalPeakPriceEvent  
InitiateCriticalPeakPriceEventToGroup  
CancelCriticalPeakPriceEvent  
CancelCriticalPeakPriceEventToGroup

1. Added messageType calling parameter of type IHDMessageType to IHDMessageStatusNotification on CB\_SERVER, MDM\_SERVER and NOT\_SERVER
2. GetAllDRProgramsByStatus methods marked as deprecated and to be removed in v5.0. Replaced by GetDRProgramsByStatus method on SCADA\_SERVER.
3. Added GetDRProgramEnrollmentsByStatus method on CB\_SERVER
4. Added messageConfirmedTime (DateTime) and errorString (string) to the end of the calling parameter list of IHDMessageConfirmedNotification on CB\_Server, MDM\_Server, NOT\_Server.

**Version 4.1.5 Release – Issued 3/1/2012.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**UML and Schema Changes:**

1. Corrected HANDeviceID, HANInterfaceID, HANGroupID, and HANSecurityToken to inherit from stringType by extension.
2. Added meterID to the ppmLocation.
3. Changed ppmLocation.rateCode to be ppmLocation.rate.
4. Modified rate object to inherit from mspObject, added rateComponents and TOUSchedules.
5. Deleted rateInfo object.
6. Added simpleType rateCode and replaced rate.rateCode and rateComponent.rateCode, previously of string type, to be of type rateCode.
7. Added rateCode to electricService, gasService, waterService, propaneService and otherService. (Note: In V4.2, these will all inherit from the new mspUsagePoint, which would carry a rateCode element and these individual rateCode elements will be removed).
8. Changed inHomeDisplayBillingMessage.currentRate to be of type rateCode .
9. Changed usageInstance.rate to be of type rateCode.
10. Changed rateComponent to extend from floatType.
11. Added timeStamp to eventInstance.
12. Added eventMonitoringList, meterConfigurationStatus, thresholdNotificationList and thresholdMonitoringList message payloads.
13. Added receivedIHDs and endDeviceShipment.receivedIHDs.
14. Added DRProgram and DRProgramEnrollment.
15. Added “ServiceReconnected” to the enumeration list for CDReasonCode.
16. Added meterConnectionStatus simpleType with enum of: [Connected/Disconnected/DisconnectedNon-Pay/Other/Unknown].
17. Added meterConnectionStatus to the end of electricMeter, gasMeter, waterMeter, propaneMeter and otherMeter.
18. Added CDEnabledResponse
19. Added a timestamp to electricMeterExchange, waterMeterExchange, gasMeterExchange, propaneMeterExchange, and otherMeterExchange.
20. Made meterID.objectID mandatory.
21. Added otherMeters to the “meters” container object.
22. Deprecated the use of inHomeDisplayBillingMessage.inHomeDisplayID.

**Web Service Method Changes:**

1. Added InitiateMeterEventMonitoring to MR\_Server and MDM\_Server (*for use case MSP.MR:50.120*).
2. Added CancelMeterEventMonitoring to MR\_Server and MDM\_Server (*for use case MSP.MR:50.130*).
3. Add a GetMetersByMeterConnectionStatus on CB\_Server and MDM\_Server. (Use case is for OMS to query CB for meters that have been disconnected for non-payment, *MSP.OM:10.190*).
4. Add GetMeterByTransponderID on CB\_Server and MDM\_Server (*to support use case MSP.MR:60.135*).
5. Added IsCDSupported to CD\_Server and MDM\_Server *(for MSP.CAM:40.105)*.
6. Added InitiateThresholdMonitoring *(for MSP.CAM:40.220)*, AdjustThresholdMonitoring *(for MSP.CAM:40.230)*, and CancelThresholdMonitoring *(for MSP.CAM:40.240)* to MR\_Server and MDM\_Server.
7. Added ThresholdEventNotification to PPM\_Server, MDM\_Server, and NOT\_Server *(for MSP.CAM:40.108)*.
8. Added ReadingChangedNotification *(for MSP.CAM:40.125)*, OutageEventChangedNotification *(for MSP.CAM:40.210)*, and CDStatesChangedNotification *(for numerous use cases including MSP.CAM:40.130)* to PPM\_Server.
9. Added AdjustPPMBalance to CB (*for MSP.CAM:40.190*).
10. Deprecated InitiateArmCDDevice on all servers (CD\_Server and MDM\_Server).
11. Deprecated MeterExchangeNotification and PPMMeterExchangeNotification on all servers. They will be replaced with InitiateMeterExchange in Version 4.2
12. Deprecated MeterRemoveNotification on all servers. It will be replaced with MeterUninstalledNotification in Version 4.2.
13. DeprecatedMeterRetireNotification on all servers. It will be replaced by MeterRemovedNotification in Version 4.2.
14. Fixed special characters in the annotation for RegisterForService and GetDomainNames.
15. Added new InitiateMeterExchange on MDM, OA, PPM and MR servers with the payload of meterExchanges, transactionID and responseURL (*for use case MSP.MR:60.140*).
16. Add new MeterExchangedNotification on MDM, AM, CB, PPM, and NOT servers with the payload of a meterExchanges and transactionID (*for use case MSP.MR:60.140*).
17. Add transactionID and responseURL to all instances of InsertMeterInConfigurationGroup.
18. Add transactionID to all instances of MeterInstalledNotification.
19. Add MeterConfigurationNotification on CB\_Server, MDM\_Server, AM\_Server and NOT\_Server (*for use case MSP.MR:80.50*).
20. Add RateChangedNotification to PPM\_Server, HAN\_Server, MR\_Server, MDM\_Server, and NOT\_Server *(for MSP.CAM:30.140)*.
21. Add InitiateMeterInstallation to MDM\_Server, MR\_Server, and PPM\_Server (*for use case MSP.MR:60.115*).
22. Deprecate InHomeDisplayBillingMessageNotification in all servers. Replace it with a new message called InitiateInHomeDisplayBillingMessage (*for use case MSP.DR:40.100)* and CancelInHomeDisplayBillingMessage *(for use case MSP.DR:40.143)*, both to be added to the HAN\_Server, MDM\_Server, and PPM\_Server*.*
23. Replace HANGroupID with HANDeviceID and HANInterfaceID in calling parameters on CancelInHomeDisplayMessage and correct message annotation (bug fix), on HAN\_Server, MDM\_Server, and PPM\_Server.
24. Add GetCustomersAffectedByOutage to MDM\_Server and interface chart.
25. Add ServiceLocationChangedNotification to HAN\_Server and interface chart.
26. Added DRProgramAddNotification to CB, DR, and NOT (for use case MSP.DR:80.100).
27. Added DRProgramChangedNotification to CB, DR, and NOT (for use case MSP.DR:80.110 and MSP.DR:80.130).
28. Added DRProgramRescindedNotification to CB, DR, and NOT (for use case MSP.DR:80.120).
29. Added GetAllDRPrograms to SCADA (for use case MSP.DR:80.140).
30. Added GetDRProgramsByStatus to SCADA (for use case MSP.DR:80.150).
31. *Added* DRProgramEnrollmentNotification to SCADA, DR and NOT*(for use case MSP.DR:80.160).*
32. *Added* DRProgramUnenrollmentNotification to SCADA, DR and NOT*(for use case MSP.DR:80.170).*
33. Added transactionID and meterReading to UsageMonitoringNotification in CB\_Server, MDM\_Server, and NOT\_Server. The addition of the transactionID permits linking this notification method with the previously sent InitiateUsageMonitoring method call. The addition of the array of meterReading permits sending the actual meter dial reading or usage since the InitiateUsageMonitoring call was made. Ideally the payload would be structured as an array of usageMonitoringItem with a mandatory meterID and an optional meterReading to link the two data elements, but this would be a breaking change for Version 4.1. The breaking change will be implemented in Version 4.2, however, in the meantime, annotation is include that requires the use of the meterReading.meterID element when meterReadings are provided. This requirement would permit linking the meterReading instances with the instances of meterID also included in the payload.
34. Add lastReceived parameter to GetBillingData.
35. Add InitiateHistoricalMeterReadingsByMeterIDAndDate to MR\_Server, and MDM\_Server (for use case MSP.MR:10.170).
36. Added transactionID to the MeterTestNotification.
37. Added GetSupportedMeterEventCodes to MR and MDM. (for use case MR:50.140).
38. Added InitiateBillingDeterminants to MDM (for use cases MR:10.200 and MR:10.210).
39. Added LMDeviceInstalledNotification to MDM\_Server.
40. Added responseURL parameter to all instances of the following messages:
    1. CancelInHomeDisplayMessage
    2. CancelInHomeDisplayMessageToGroup
    3. InitiateHANCommissioning
    4. InitiateHANPricing
    5. InitiateHANPricingRequest
    6. InitiateIHDCapabilitySettings
    7. InitiateIHDCapabilitySettingsToGroup
    8. InitiateInHomeDisplayMessage
    9. InitiateInHomeDisplayMessageToGroup
    10. InitiateManufacturerSpecificCommand
    11. InitiateManufacturerSpecificCommandToGroup
    12. InitiateThermostatConfiguration
    13. InitiateThermostatConfigurationRequest
    14. InitiateThermostatSchedule
    15. InitiateThermostatScheduleRequest
41. Added transactionID parameter to all instances of the following messages:
    1. InitiateHANRegistrationStatusRequest.
42. Added an optional HANInterfaceID to the following messages:
    1. DemandResponseSetupNotification
    2. TemperatureTiersCHangedNotification
    3. LoadCycleTiersNotification
    4. ManufacturerSpecificCommandNotification
    5. ThermostatScheduleConfirmedNotification
    6. ThermostatConfigurationNotification
    7. IHDMessageStatusNotification
    8. IHDMessageConfirmedNotification
    9. IHDCapabilitySettingsNotification
    10. CancelCriticalPeakPriceEvent
    11. InitiateCriticalPeakPriceEvent
    12. InitiateDemandResponseSetup
    13. InitiateIHDCapabilitySettings
    14. InitiateInHomeDisplayMessage
    15. InitiateManufacturerSpecificCommand
    16. InitiateThermostatSchedule
    17. InitiateThermostatScheduleRequest
    18. InitiateThermostatConfiguration
    19. InitiateThermostatConfigurationRequest

**Version 4.1.4 Release Candidate – Issued 10/15/2011.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**UML and Schema Changes:**

1. Corrected mspCPSM schemaLocation in UML class model.
2. Added Customer, Service, Premise and Parcel class diagram to the UML model in EA. [(ID0000042)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=42)
3. A new UML Class diagram for “Abstract Class Inheritance” has been added to the UML model. [(ID0000043)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=43)
4. Added TOUSChedules to configuredReadingType [(ID0000106)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=106)
5. Corrected spelling of usageInstance.unitPrefeix to usageInstance.unitPrefix. [(ID0000107)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=107)
6. Made objectRef.noun and objectRef.objectID required rather than optional [(ID0000108)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=108)
7. Added a new assetRef [(ID0000109)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=109), assets container class [(ID0000110)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=110)
8. Added new objects:
   1. Added TOUSchedules, TOUSchedule, effectiveDate, daysOfWeek, bins, bin, dayLabel, dayNumber, monthNumber, exceptionDays [(ID0000105)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=105)
   2. HANInterfaceID [(ID0000131)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=131)
   3. HANDeviceID [(ID0000133)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=133)
   4. HANGroupID [(ID0000134)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=134)
   5. HANSecurityToken [(ID0000135)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=135)
   6. HANRegistration, HANRegistrationStatus [(ID0000140)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=140)
   7. InitiateHANRegistrationStatus [(ID0000144)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=144)
   8. IHDMessageStatus [(ID0000158)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=158)
   9. inHomeDisplayCapabilitySetting [(ID0000163)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=163)
   10. priceBin, priceTier, and priceTierStructure [(ID0000166)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=166)
   11. temperatureTier and temperatureTierStructure [(ID0000167)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=167)
   12. loadCycleTier and loadCycleTierStructure [(ID0000168)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   13. thermostatSchedule, thermostatScheduleDay, thermostatScheduleTime and days [(ID0000175)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=175)
   14. thermostatConfiguration [(ID0000180)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   15. thermostatCurrentConfiguration [(ID0000181)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   16. tunnelCommandContent [(ID0000185)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   17. thermostat [(ID0000189)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   18. HANDeviceGroup [(ID0000203)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   19. HANCommission and commissionStatus enumeration [(ID0000212)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   20. demandRepsonseParameters [(ID0000215)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   21. demandResponseEvent [(ID0000218)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   22. demandResponseEventStatus [(ID0000219)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   23. criticalPeakPriceEvent [(ID0000229)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   24. criticalPeakPriceEventStatus [(ID0000230)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   25. thermostatMode [(ID0000279)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
   26. thermostatFan [(ID0000280)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
9. Add “InTransition” and “PowerLimitation” to RCDState [(ID0000264)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
10. Add optional timestamp element to CDState and CDStateChange classes [(ID0000265)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
11. Add “CancelPowerLimitation” to loadActionType [(ID0000281)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=168)
12. Corrected the spelling on both element and class maintenanceOrderList [(ID0000112)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=112)
13. Corrected the spelling of priority on phoneNumber.priorityOrder [(ID0000113)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=113)
14. Modified bufferedObjectCollection class [(ID0000150)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=150)
15. Corrected assignment.timeToLive to be of type msp:duration rather than xs:duration.
16. Corrected sectionalizerEntry.resetTime to be of type msp:duration rather than xs:duration.
17. Renamed V4.1.3 demandResponseEvent to be demandResponseEventDeprecated and changed annotation. [(ID0000216)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
18. Deprecated the ZigBee\* elements. [(ID0000217)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)

**Web Service Method Changes:**

1. The return type for the GetConfigurationGroupMembers has been changed to configurationGroup [(ID0000054)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=54)
2. Renamed the method GetAccountByMeterIDAndServiceType on CB\_server to GetAccountByMeterID to match the usage on MDM Server [(ID0000055)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=55)
3. Added missing methods to MDM Server from PPM Server [(ID0000056)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=56)
   1. AdjustPPMBalance
   2. ChargeableDeviceChangedNotification
   3. CommitPaymentTransaction
   4. EnrollPPMCustomer
   5. PPMMeterExchangeNotification
   6. UnenrollPPMCustomer
   7. GetPrePayStatus
4. Added missing methods to MDM Server from CB Server [(ID0000057)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=57)
5. GetAllOtherMeters
6. GetAllServiceLocations
7. GetBilledUsage
8. GetBillingData
9. GetBillingDetail
10. GetChargeableDevicesByAccountNumber
11. GetIHDGroupMembers
12. GetIHDGroupNames
13. GetIHDGroupNamesbyInHomeDisplayID
14. GetMeterHistoryByMeterID
15. GetPPMBalanceAdjustments
16. GetPPMCustomer
17. GetPPMPayments
18. GetServiceOrderByServiceOrderID
19. GetServiceOrdersByServiceLocation
20. GetServiceOrdersByStatus
21. Added missing methods to MDM Server from SCADA Server [(ID0000058)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=58),
    1. SCADAAnalogChangedNotification
    2. SCADAAnalogChangedNotificationByPointID
    3. SCADAAnalogChangedNotificationForPower
    4. SCADAAnalogChangedNotificationForVoltage
    5. SCADAPointChangedNotification
    6. SCADAPointChangedNotificationForAnalog
    7. SCADAPointChangedNotificationForStatus
    8. SCADAStatusChangedNotification
    9. SCADAStatusChangedNotificationByPointID
22. Added missing methods to MDM Server from DR Server [(ID0000059)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=59),
    1. GetAllLoadManagementDevices
    2. GetAllSubstationLoadControlStatuses
    3. GetAmountOfControllableLoad
    4. GetAmountOfControlledLoad
    5. GetLoadManagementDeviceByMeterID
    6. GetLoadManagementDeviceByServiceLocationID
    7. IsLoadManagementActive
    8. LMDeviceAddNotification
    9. LMDeviceChangedNotification
    10. LMDeviceExchangeNotification
    11. LMDeviceInstalledNotification
    12. LMDeviceRemoveNotification
    13. LMDeviceRetireNotification
23. Added missing methods to MDM Server from EA Server [(ID0000060)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=60)+ [(ID0000062)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=62),
    1. GetCircuitElementByObject
    2. GetMeterConnectivityByMeterID
24. Added missing methods to MDM Server from OA Server [(ID0000061)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=61).
    1. GetAllActiveOutageEvents
    2. GetOutageEvent
25. Added missing methods to GIS Server from EA Server [(ID0000062)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=62)
    1. GetMeterConnectivityByMeterID
26. Changed the Method/Service Names
    1. EnableReadingSchedule to EnableReadingSchedules (on MDM\_Server to match usage on MR\_Server) [(ID0000063)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=63)
    2. GetAccountByCustomerID to GetAccountsByCustomerID (on MDM\_Server to match usage on CB\_Server) [(ID0000064)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=64)
    3. ModifyCBDataForServiceLocation to ModifyCBDataServiceLocations (on MDM\_Server to match usage on CB\_Server) [(ID0000065)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=65)
    4. ModifyCBDataForMeter to ModifyCBDataForMeters (on MDM\_Server to match usage on CB\_Server) [(ID0000066)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=66)
    5. Changed AnalogChangedNotificationByPointID method on all Servers to generalize publisher/subscriber relationships [(ID0000116)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=116)
    6. Changed StatusChangedNotificationByPointID method on all Servers to generalize publisher/subscriber relationships [(ID0000117)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=117)
    7. Corrected misspelling of “Accumulated” from AccumulatedValueChangedNotification method name in various servers (SCADA, DA and NOT Servers) [(ID0000119)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=119)
    8. Corrected misspelling of “GetLatestReading” from method name in MDM\_Server [(ID0000120)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=120)
    9. Corrected the spelling of GetCircuitElementNearLatLong on OA\_Server [(ID0000137)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=137)
    10. Changed the method from GetPropaneMeterByAccountNumber to GetPropaneMetersByAccountNumber on CB and MDM Servers [(ID0000139)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=139) and change the spelling of GetPropaneMeterByAccountNumber entry on the CB and MDM Server interface charts [(ID0000148)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=148)
    11. Replace InitiateTaskGeneration with InitiateWorkRequest on WTG\_Server [(ID0000145)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=145)
27. Changes to AM\_Server
    1. Added new method GetMeterHistoryByMeterID [(ID0000068)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=68)
    2. Added new method GetAssetRefByObjectRef [(ID0000111)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=111)
    3. Added new method GetAssetByAssetRef [(ID0000111)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=111)
    4. Added new method GetAssetsByAssetField [(ID0000111)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=111)
    5. Added new method ThermostatAddNotification [(ID0000190)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    6. Added new method ThermostatRemoveNotification [(ID0000191)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    7. Added new method EstablishHANDeviceGroup [(ID0000197)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    8. Added new method DeleteHANDeviceGroup [(ID0000198)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    9. Added new method InsertIntoHANDeviceGroup [(ID0000199)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    10. Added new method RemoveFromHANDeviceGroup [(ID0000200)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    11. Added new method EstablishIHDGroup [(ID0000205)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    12. Added new method DeleteIHDGroup [(ID0000206)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    13. Added new method InsertInHomeDisplayInIHDGroup [(ID0000207)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    14. Added new method RemoveInHomeDisplayFromIHDGroup [(ID0000208)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
28. Changes to CB\_Server
    1. Added new method HANRegistrationNotification [(ID0000141)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=141)
    2. Added new method IHDMessageStatusNotification [(ID0000159)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=159)
    3. Added new method IHDMessageConfirmedNotification [(ID0000162)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=162)
    4. Added new method IHDCapabilitySettingsNotification [(ID0000165)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=165)
    5. Added new method PricingTiersChangedNotification [(ID0000170)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=170)
    6. Added new method TemperatureTiersChangedNotification[(ID0000171)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=171)
    7. Added new method LoadCycleTiersChangedNotification [(ID0000172)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=172)
    8. Added new method HANPricingNotification [(ID0000174)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=174)
    9. Added new method ThermostatScheduleNotification [(ID0000177)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    10. Added new method ThermostatConfigurationNotification [(ID0000183)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    11. Added new method ManufacturerSpecificCommandNotification [(ID0000187)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    12. Added new method ThermostatScheduleConfirmedNotification [(ID0000188)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    13. Added new method GetHANDeviceGroupNames [(ID0000201)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    14. Added new method GetHANDeviceGroupMembers [(ID0000202)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    15. Added new method GetHANDeviceGroupNamesByHANDeviceID [(ID0000204)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    16. Added new method GetIHDGroupNames [(ID0000209)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    17. Added new method GetIHDGroupMembers [(ID0000210)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    18. Added new method GetIHDGroupNamesByInHomeDisplayID [(ID0000211)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    19. Added new method HANCommissioningNotification [(ID0000214)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    20. Added new method DemandResponseSetupNotification [(ID0000221)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    21. Added new method DemandResponseEventNotification [(ID0000223)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    22. Added new method CriticalPeakPriceEventNotification [(ID0000234)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
29. Changes to DR\_Server
    1. Added new method AnalogChangedNotificationByPointID [(ID0000118)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=118)
    2. Added new method StatusChangedNotificationByPointID [(ID0000118)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=118)
    3. Added new method EstablishHANDeviceGroup [(ID0000197)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    4. Added new method DeleteHANDeviceGroup [(ID0000198)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    5. Added new method InsertIntoHANDeviceGroup [(ID0000199)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    6. Added new method RemoveFromHANDeviceGroup [(ID0000200)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    7. Added new method GetHANDeviceGroupNames [(ID0000201)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    8. Added new method GetHANDeviceGroupMembers [(ID0000202)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    9. Added new method GetHANDeviceGroupNamesByHANDeviceID [(ID0000204)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    10. Added new method GetIHDGroupNames [(ID0000209)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    11. Added new method GetIHDGroupMembers [(ID0000210)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    12. Added new method GetIHDGroupNamesByInHomeDisplayID [(ID0000211)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    13. Added new method InitiateDemandResponseSetup [(ID0000220)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    14. Added new method InitiateDemandResponseEvent [(ID0000222)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    15. Added new method CancelDemandResponseEvent [(ID0000224)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    16. Added new method InitiateDemandResponseEventStatusRequest [(ID0000225)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    17. Added new method InitiateDemandResponseEventToGroup [(ID0000226)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    18. Added new method CancelDemandResponseEventToGroup [(ID0000227)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    19. Added new method InitiateDemandResponseEventStatusRequestToGroup [(ID0000228)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    20. Added new method InitiateCriticalPeakPriceEvent [(ID0000233)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    21. Added new method CancelCriticalPeakPriceEvent [(ID0000235)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    22. Added new method InitiateCriticalPeakPriceEventToGroup [(ID0000236)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    23. Added new method CancelCriticalPeakPriceEventToGroup [(ID0000237)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
30. Changes to GV\_Server
    1. Added new method AnalogChangedNotificationByPointID [(ID0000118)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=118)
    2. Added new method StatusChangedNotificationByPointID [(ID0000118)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=118)
31. Changes to HAN\_Server
    1. Added new method InitiateHANRegistration [(ID0000138)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=138)
    2. Added new method CancelHANRegistration [(ID0000142)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=143)
    3. Added new method InitiateHANRegistrationStatusRequest [(ID0000143)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=138)
    4. Deprecated InHomeDisplayMessageNotification [(ID0000156)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=156)
    5. Added new method InitiateInHomeDisplayMessage [(ID0000157)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=157)
    6. Added new method CancelInHomeDisplayMessage [(ID0000160)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=160)
    7. Added new method InitiateInHomeDisplayMessageToGroup[(ID0000161)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=161)
    8. Added new method InitiateIHDCapabilitySettings [(ID0000164)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=164)
    9. Added new method InitiateHANPricing [(ID0000168)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=164)
    10. Added new method InitiateHANPricingRequest[(ID0000173)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=173)
    11. Added new method InitiateThermostatSchedule [(ID0000176)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    12. Added new method InitiateThermostatScheduleRequest [(ID0000178)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    13. Added new method CancelInHomeDisplayMessageToGroup [(ID0000179)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    14. Added new method InitiateThermostatConfiguration [(ID0000182)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    15. Added new method InitiateThermostatConfigurationRequest [(ID0000184)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    16. Added new method InitiateManufacturerSpecificCommand [(ID0000186)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    17. Added new method ThermostatAddNotification [(ID0000190)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    18. Added new method ThermostatRemoveNotification [(ID0000191)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    19. Added new method EstablishHANDeviceGroup [(ID0000197)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    20. Added new method DeleteHANDeviceGroup [(ID0000198)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    21. Added new method InsertIntoHANDeviceGroup [(ID0000199)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    22. Added new method RemoveFromHANDeviceGroup [(ID0000200)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    23. Added new method GetHANDeviceGroupNames [(ID0000201)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    24. Added new method GetHANDeviceGroupMembers [(ID0000202)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    25. Added new method GetHANDeviceGroupNamesByHANDeviceID [(ID0000204)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    26. Added new method GetIHDGroupNames [(ID0000209)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    27. Added new method GetIHDGroupMembers [(ID0000210)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    28. Added new method GetIHDGroupNamesByInHomeDisplayID [(ID0000211)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    29. Added new method InitiateHANCommissioning [(ID0000213)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    30. Added new method InitiateManufacturerSpecificCommandToGroup [(ID0000231)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    31. Added new method InitiateIHDCapabilitySettingsToGroup [(ID0000232)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
32. Changes to INSP\_Server
    1. Added new method GetActiveAssessmentLocations [(ID0000146)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=146)
    2. Removed GetCircuitElementNearLatLong [(ID0000151)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=151)
33. Changes to MDM\_Server
    1. Added new method AnalogChangedNotificationByPointID [(ID0000118)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=118)
    2. Added new method StatusChangedNotificationByPointID [(ID0000118)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=118)
    3. Added new method InitiateHANRegistration [(ID0000138)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=138)
    4. Added new method HANRegistrationNotification [(ID0000141)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=141)
    5. Added new method CancelHANRegistration [(ID0000142)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=143)
    6. Added new method InitiateHANRegistrationStatusRequest [(ID0000143)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=138)
    7. Removed listing for obsolete method GetAllActiveCalls [(ID0000067)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=67)
    8. Removed listing for obsolete method GetCustomerByMeterIDAndServiceType [(ID0000067)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=67)
    9. Removed listing for obsolete method MeterTestTransaction [(ID0000067)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=67)
    10. Removed listing for obsolete method GetAllPropaneServiceLocations [(ID0000067)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=67)
    11. Deprecated InHomeDisplayMessageNotification [(ID0000156)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=156)
    12. Added new method InitiateInHomeDisplayMessage [(ID0000157)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=157)
    13. Added new method IHDMessageStatusNotification [(ID0000159)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=159)
    14. Added new method CancelInHomeDisplayMessage [(ID0000160)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=160)
    15. Added new method InitiateInHomeDisplayMessageToGroup[(ID0000161)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=161)
    16. Added new method IHDMessageConfirmedNotification [(ID0000162)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=162)
    17. Added new method InitiateIHDCapabilitySettings [(ID0000164)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=164)
    18. Added new method IHDCapabilitySettingsNotification [(ID0000165)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=165)
    19. Added new method InitiateHANPricing [(ID0000168)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=164)
    20. Added new method PricingTiersChangedNotification [(ID0000170)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=170)
    21. Added new method TemperatureTiersChangedNotification[(ID0000171)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=171)
    22. Added new method LoadCycleTiersChangedNotification [(ID0000172)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=172)
    23. Added new method InitiateHANPricingRequest[(ID0000173)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=173)
    24. Added new method HANPricingNotification [(ID0000174)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=174)
    25. Added new method InitiateThermostatSchedule [(ID0000176)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    26. Added new method ThermostatScheduleNotification [(ID0000177)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    27. Added new method InitiateThermostatScheduleRequest [(ID0000178)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    28. Added new method CancelInHomeDisplayMessageToGroup [(ID0000179)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    29. Added new method InitiateThermostatConfiguration [(ID0000182)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    30. Added new method ThermostatConfigurationNotification [(ID0000183)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    31. Added new method InitiateThermostatConfigurationRequest [(ID0000184)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    32. Added new method InitiateManufacturerSpecificCommand [(ID0000186)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    33. Added new method ManufacturerSpecificCommandNotification [(ID0000187)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    34. Added new method ThermostatScheduleConfirmedNotification [(ID0000188)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    35. Added new method ThermostatAddNotification [(ID0000190)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    36. Added new method ThermostatRemoveNotification [(ID0000191)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    37. Added new method EstablishHANDeviceGroup [(ID0000197)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    38. Added new method DeleteHANDeviceGroup [(ID0000198)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    39. Added new method InsertIntoHANDeviceGroup [(ID0000199)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    40. Added new method RemoveFromHANDeviceGroup [(ID0000200)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    41. Added new method GetHANDeviceGroupNames [(ID0000201)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    42. Added new method GetHANDeviceGroupMembers [(ID0000202)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    43. Added new method GetHANDeviceGroupNamesByHANDeviceID [(ID0000204)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    44. Added new method GetIHDGroupNames [(ID0000209)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    45. Added new method GetIHDGroupMembers [(ID0000210)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    46. Added new method GetIHDGroupNamesByInHomeDisplayID [(ID0000211)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    47. Added new method InitiateHANCommissioning [(ID0000213)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    48. Added new method HANCommissioningNotification [(ID0000214)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    49. Added new method InitiateDemandResponseSetup [(ID0000220)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    50. Added new method DemandResponseSetupNotification [(ID0000221)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    51. Added new method InitiateDemandResponseEvent [(ID0000222)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    52. Added new method DemandResponseEventNotification [(ID0000223)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    53. Added new method CancelDemandResponseEvent [(ID0000224)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    54. Added new method InitiateDemandResponseEventStatusRequest [(ID0000225)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    55. Added new method InitiateDemandResponseEventToGroup [(ID0000226)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    56. Added new method CancelDemandResponseEventToGroup [(ID0000227)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    57. Added new method InitiateDemandResponseEventStatusRequestToGroup [(ID0000228)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    58. Added new method InitiateManufacturerSpecificCommandToGroup [(ID0000231)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    59. Added new method InitiateIHDCapabilitySettingsToGroup [(ID0000232)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    60. Added new method InitiateCriticalPeakPriceEvent [(ID0000233)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    61. Added new method CriticalPeakPriceEventNotification [(ID0000234)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    62. Added new method CancelCriticalPeakPriceEvent [(ID0000235)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    63. Added new method InitiateCriticalPeakPriceEventToGroup [(ID0000236)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    64. Added new method CancelCriticalPeakPriceEventToGroup [(ID0000237)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
34. Changes to NOT\_Server
    1. Added new method AddAttachmentToWorkOrder [(ID0000132)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=132)
    2. Added new method HANRegistrationNotification [(ID0000141)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=141)
    3. Added new method OutageReasonChangedNotification [(ID0000149)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=149)
    4. Added new method OutageReasonContainerChangedNotification [(ID0000149)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=149)
    5. Added new method UsageMonitoringNotification [(ID0000154)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=154)
    6. Deprecated InHomeDisplayMessageNotification [(ID0000156)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=156)
    7. Added new method IHDMessageStatusNotification [(ID0000159)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=159)
    8. Added new method IHDMessageConfirmedNotification [(ID0000162)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=162)
    9. Added new method IHDCapabilitySettingsNotification [(ID0000165)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=165)
    10. Added new method PricingTiersChangedNotification [(ID0000170)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=170)
    11. Added new method TemperatureTiersChangedNotification[(ID0000171)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=171)
    12. Added new method LoadCycleTiersChangedNotification [(ID0000172)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=172)
    13. Added new method HANPricingNotification [(ID0000174)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=174)
    14. Added new method ThermostatScheduleNotification [(ID0000177)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    15. Added new method ThermostatConfigurationNotification [(ID0000183)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    16. Added new method ManufacturerSpecificCommandNotification [(ID00001187)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    17. Added new method ThermostatScheduleConfirmedNotification [(ID0000188)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    18. Added new method ThermostatAddNotification [(ID0000190)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    19. Added new method ThermostatRemoveNotification [(ID0000191)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
    20. Added new method HANCommissioningNotification [(ID0000214)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    21. Added new method DemandResponseSetupNotification [(ID0000221)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    22. Added new method DemandResponseEventNotification [(ID0000223)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    23. Added new method CriticalPeakPriceEventNotification [(ID0000234)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
35. Changes to OA\_Server
    1. Added new method AnalogChangedNotificationByPointID [(ID0000118)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=118)
    2. Added new method StatusChangedNotificationByPointID [(ID0000118)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=118)
    3. Added new method DiscardOutage [(ID0000115)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=115)
36. Changes to PPM\_Server
    1. Deprecated InHomeDisplayMessageNotidication [(ID0000156)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=156)
    2. Added new method MeterRetireNotification [(ID0000121)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=121)
    3. Added new method MeterExchangeNotification [(ID0000130)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=130)
    4. Added new method InitiateInHomeDisplayMessage [(ID0000157)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=157)
    5. Added new method CancelInHomeDisplayMessage [(ID0000160)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=160)
    6. Added new method InitiateInHomeDisplayMessageToGroup[(ID0000161)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=161)
    7. Added new method InitiateIHDCapabilitySettings [(ID0000164)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=164)
    8. Added new method InitiateHANPricing [(ID0000169)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=169)
    9. Added new method InitiateHANPricingRequest[(ID0000173)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=173)
    10. Added new method CancelInHomeDisplayMessageToGroup [(ID0000179)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=173)
    11. Added new method InitiateManufacturerSpecificCommand [(ID0000186)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=173)
    12. Added new method InitiateManufacturerSpecificCommandToGroup [(ID0000231)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
    13. Added new method InitiateIHDCapabilitySettingsToGroup [(ID0000232)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
37. Made changes to RestoreOutage on OA\_Server to return array of errorObjects [(ID0000114)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
38. Added transactionID to all InHomeDisplayAddNotification [(ID0000192)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
39. Added transactionID to all InHomeDisplayRemoveNotification [(ID0000193)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
40. Added transactionID to all LMDeviceAddNotification[(ID0000194)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
41. Added transactionID to all LMDeviceRemoveNotification[(ID0000195)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
42. Added transactionID to all LMDeviceChangedNotification[(ID0000196)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
43. Changed CDStateChangedNotification to carry a CDStateChange object instead of a meterID and stateChange parameters [(ID0000252)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
44. Changed workOrder calling parameter in WorkOrderChangedNotification in EA server to an array of workOrder [(ID0000253)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
45. Added GetReadingsByMeterIDListAndFieldNameIntervalData method to MR\_Server, MDM\_Server, and MR/MDM interface charts. [(ID0000266)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
46. Changed return type on GetCDMeterState to be CDState on CD\_Server and MDM\_Server. [(ID0000267)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
47. Added CDStatesChangedNotification to OA\_Server and OA interface chart. Edit MDM and NOT charts. [(ID0000268)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
48. Added "OPT" to NOT column of AM\_Server for WorkOrderChangedNotificatioToGIS method. [(ID0000269)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
49. Added lastReceived parameter to all instances of GetUplineCircuitElements, GetChildCircuitElements, and GetParentCircuitElements. [(ID0000271)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
50. Added OutageReasonChangedNotification and OutageReasonContainerChangedNotification to MDM from OA [(ID0000272)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
51. Corrected implementation of GetElectricalEquipment method on GIS\_Server [(ID0000273)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
52. Added GetMeterConnectivityByMeterID to MDM from EA [(ID0000274)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
53. Changed return type to an array of errorObjects in methods on OA (RestoreOutage), WTG (NumberCreatedNotification), and WTO (NumberCreatedNotification) [(ID0000275)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
54. Added transactionID to MeterEventNotification in AM, CB, MDM, NOT servers [(ID0000276)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
55. Removed formattedBlockTemplateName parameter from GetLatestMeterReadingsByMeterGroupIntervalData method [(ID0000282)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
56. Changed GetServiceLocationIDByAccountNumber method in CB\_Server to return an array of strings [(ID0000283)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
57. Change calling parameter on GetServiceOrderByServiceOrderID method to be serviceOrderID rather than serviceLocationID in CB\_Server and MDM\_Server [(ID0000284)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
58. Removed incorrect text about error handling from method descriptions in CB\_Server and MDM\_Server [(ID0000285)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
59. Added text about transactionID usage to descriptions for UpdateProjects and ProjectChangedNotification methods [(ID0000286)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
60. Added transactionID calling parameter to InitiateUsageMonitoring method in MDM and MR servers [(ID0000287)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
61. Change the return type on all instances of GetAllInHomeDisplays to be an array of inHomeDisplay rather than a readingSchedule. [(ID0000270)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)
62. Added lastReceived parameter to GetAllMetersByAccountNumber method in CB, MDM [(ID0000288)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=114)

**Version 4.1.3 Release – Issued 2/15/2011.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**UML and Schema Changes:**

1. Changed the version namespace in all of the schemas to be <http://www.multispeak.org/Version_4.1_Release> instead of 4.1.x\_Release. Similar changes were made to CPSM and GML namespaces. [(ID:0000019)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=19)
2. Deleted unused neutralConductorList complexType. [(ID:0000007)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=7)
3. Replaced existing MDM Interface chart with the new updated document. [(ID: 0000021)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=21)
4. Removed interface numbers from all interface charts. [(ID:0000018)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=18)
5. Created GPSLocation and added to AVLState and AVLPosition and marked the GPS element as being optional and deprecated. [(ID:0000027)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=27)
6. Added new GPSLocation to mspPointObject, inspection, and bufferedPoint and marked the current gpsPoint as being deprecated. [(ID:0000028)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=28)
7. Replaced the existing gpsLocation element with the new GPSLocation in the mspPointObject and station. [(ID:0000029)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=29)
8. Added parentMeterList to electricMeter. [(ID: 0000023)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=23)
9. Added subMeterList to electricMeter. [(ID:0000022)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=22)
10. Deprecated specialNeeds and annotated corresponding places. [(ID:0000024)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=24)
11. Changed the annotation on electricService.specialNeeds to be identical to the annotation on customer.specialNeeds. [(ID:0000037)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=37)
12. Corrected the annotation on GPSLocation and all of its elements, both on the complexType and each use as an element. [(ID:0000038)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=38)
13. Corrected annotation on AVLState.GPS and AVLPosition.gps [(ID:0000039)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=39)
14. Deleted the default=2 tagged value on otherService.customerID. [(ID:0000040)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=40)
15. Corrected targetnamespace list on MultiSpeak container object. [(ID:0000041)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=41)

**Web Service Method Changes:**

1. Added UsageMonitoringNotification to CB\_Server and MDM\_Server. [(ID0000020)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=20)+[(ID0000025)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=25),
2. Added responseURL parameter to InitiateUsageMonitoring on MR\_Server and MDM\_Server and modify annotation to method. [(ID0000026)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=26)
3. Changed the spelling of InitiateMeterReadingByMeterID to be InitiateMeterReadingsByMeterID on MDM\_Server to match the usage on the MR\_Server. [(ID0000032)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=32)
4. Removed GetCustomerByMeterIDAndServiceType from CB\_Server. [(ID0000033)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=33)
5. Removed serviceType parameter from the following methods:
   1. CancelUsageMonitoring (on MDM\_Server to match usage on MR\_Server)
   2. InitiateUsageMonitoring (on MDM\_Server to match usage on MR\_Server)
   3. CancelDisconnectedStatus (on MDM\_Server to match usage on MR\_Server)
   4. InitiateDisconnectedStatus (on MDM\_Server to match usage on MR\_Server)
   5. InsertMeterInMeterGroup (on MDM\_Server to match usage on MR\_Server)
   6. RemoveMetersFromMeterGroup (on MDM\_Server to match usage on MR\_Server)
   7. InsertMeterInConfigurationGroup (on MDM\_Server to match usage on MR\_Server)
   8. RemoveMetersFromConfigurationGroup (on MDM\_Server to match usage on MR\_Server)
   9. InitiateMeterReadingByMeterIDAndFieldName (on both MR\_Server and MDM\_Server)
   10. InitiateMeterReadingsByMeterID (on both MR\_Server and MDM\_Server)
   11. GetLatestReadingsByMeterIDList (on MR\_Server to match usage on MDM\_Server)
   12. GetReadingsByMeterIDAndFieldName (on MR\_Server to match usage on MDM\_Server)
   13. GetLatestReadingByMeterIDAndFieldName (on MR\_Server to match usage on MDM\_Server)
   14. GetReadingsByMeterID (on MR\_Server to match usage on MDM\_Server)
   15. GetLPDataByMeterID (on MR\_Server to match usage on MDM\_Server)
   16. GetLPReadingsByMeterIDFormattedBlock (on MR\_Server to match usage on MDM\_Server)
   17. GetCustomerByMeterID (on both MDM\_Server and CB\_Server)
   18. GetMeterGroupNamesByMeterID (on both MDM\_Server and CB\_Server)
   19. GetReadingByMeterIDIntervalData (on both MR\_Server and MDM\_Server)
   20. GetReadingByMeterIDFormattedBlock (on both MR\_Server and MDM\_Server)
   21. GetLatestReadingByMeterID (on MDM\_Server to match usage on MR\_Server)
   22. GetServiceLocationByMeterID (on both MDM\_Server and CB\_Server)
   23. GetLatestReadingsByMeterListFormattedBlock (on both MR\_Server and MDM\_Server)
   24. GetLatestReadingsByMeterListIntervalData (on both MR\_Server and MDM\_Server)
   25. InitiatePlannedOutage (on MDM\_Server to match usage on MR\_Server)

[(ID0000034)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=34)

**Other Changes:**

1. Created these 4.1.3 Release notes. [(ID:0000030)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=30)
2. Created 4.1.3 Release package. [(ID:0000031)](https://crnsgd.saicwebhost.net/mantisbt/view.php?id=31)

**Version 4.1.2 Release – Issued 1/10/2011.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**UML and Schema Changes:**

1. Changed the namespace in all of the schemas to be <http://www.multispeak.org/Version_4.1.2_Release>
2. CPSM and GML namespaces are now versioned.  
   [(ID:0000003)](http://crnsgd.saicwebhost.net/mantisbt/view.php?id=3)
3. Made the mspDate simple type be built by restriction rather than as a list. [(ID: 0000004)](http://crnsgd.saicwebhost.net/mantisbt/view.php?id=4)
4. Made the priorityOrder simple type be built by restriction rather than as a list. [(ID:0000005)](http://crnsgd.saicwebhost.net/mantisbt/view.php?id=5)
5. Deleted unnecessary neutralConductorList complexType.   
   [(ID:0000007)](http://crnsgd.saicwebhost.net/mantisbt/view.php?id=7)
6. Changed the tagged value on MultiSpeak.documentType. The TaggedValue “Fixed” on MultiSpeak.documentType should not have any value.[(ID:0000013)](http://crnsgd.saicwebhost.net/mantisbt/view.php?id=13)
7. Changed the “any ##targetNamespace” on the MultiSpeak class to be “any ##targetNamespace cpsm gml cim” and changed the processContents attribute to be “strict” instead of “lax”. [(ID:0000014)](http://crnsgd.saicwebhost.net/mantisbt/view.php?id=14)

**Web Service Method Changes:**

1. Added errorString parameter to the GetFeaturesNearLatLong method on OA\_Server.  
   [(ID:0000015)](http://crnsgd.saicwebhost.net/mantisbt/view.php?id=15)
2. Changed the annotation on the PointSubscriptionList in the SCADA\_Server to be: “Client notifies SCADA of a new list of points to which it would like to subscribe. This list replaces any prior lists. The client SHALL provide the RegistrationID under which this subscription is being requested, unless the SCADA server does not support automated registration for services. If automated subscription is supported, the subscriber SHALL include the RegistrationID in the message header for this method. SCADA returns failed transactions by returning an array of errorObjects. Subscriber specifies the URL to which information is to be published by sending the responseURL. “ [(ID:0000006)](http://crnsgd.saicwebhost.net/mantisbt/view.php?id=6)

**Other Changes:**

1. Removed dependency on MHT files. PDF files are now used instead of MHT files.  
   [(ID:0000012)](http://crnsgd.saicwebhost.net/mantisbt/view.php?id=12)

**Version 4.1.1 Release – Issued 11/15/2010.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**UML and Schema Changes:**

1. Changed the namespace in all of the schemas to be <http://www.multispeak.org/Version_4.1.1_Release>
2. Added AuditID and AuditPassword to message header schema.
3. Corrected batch message header to match the web services message header.
4. Refactored intervalData object
5. Refactored accountsReceivable.
6. Added receivedDate to endDeviceShipment.
7. Added configuredReadingTypes to configurationGroup.
8. Fixed spelling of outageEvent.completed.
9. Added installedDate and removedDate to mspMeter.
10. Added bufferedObjectCollection.
11. Added domainMemberChange.
12. Corrected GPS.latitude, GPS.longitude, gpsLocation.lataitude, gpsLocation.longitude, gpsPoint.latitude, gpsLocation.altitude, gpsPoint.longitude and gpsPoint.altitude to be of type double, rather than float.
13. Added outageReasonContainer, outageReasonList, outageReasonItem, outageReportingCategory, outageReason, outageReasonCodeList, and outageReportingCode.
14. Added ServiceRestored to enumeration list for CDReasonCode.
15. Added the following elements to the electricMeterExchange, waterMeterExchange, gasMeterExchange, propaneMeterExchange, and otherMeterExchange: lastRead, lastReadDate, and averageConsumption.
16. Added “Other” and/or “Unknown” to the following enumeration lists:
    1. baseType
    2. capacitorConnectionCode
    3. swType
    4. swStatus
    5. extType
    6. readingStatus
    7. mounting
    8. wdgCode
    9. treatment
    10. regulatorWindingType
    11. nemaType
    12. qualityDescription
    13. controlStatus
    14. assignmentStatus
    15. balanceType
17. outageEvent.faultType was marked as being deprecated.
18. Added serviceLocationID, serviceID and meterID to outageCustomer.

**Web Service Method Changes:**

1. Added HistoryLogChangedNotification to OA\_Server.
2. Added transactionID to the FormattedBlockNotification in the EA\_Server to ensure consistent formatting with the same method on other servers.
3. Fixed incorrect calling parameter in GetNextNumber in FA\_Server.
4. Removed GetNextNumber and ReturnGeneratedNumber in OA\_Server.
5. Corrected ModifyCBDataforCustomer in MDM\_Sserver to carry an array of customer rather than a single customer.
6. Corrected returned parameter in PoleChangedNotification to be changedPoles rather than changedpoles in GIS\_Server.
7. Ensured consistent format of the following methods in CB\_Server and MDM\_Server:
   1. GetMeterGroupNamesByMeterID
   2. GetModifiedMeters
   3. GetModifiedServiceLocations
   4. GetServiceLocationByAccountNumber
   5. GetServiceLocationByGridLocation
   6. GetServiceLocationByMeterID
   7. GetServiceLocationByServiceStatus
   8. GetServiceLocationByShutOffDate
8. Added GetCircuitElementStatus and GetFeaturesNearLatLong to OA\_Server.
9. Added annotation to SetOutageElementStatus method on OA\_Server to recommend verifying the current status with a call to GetCircuitElementStatus before setting the status.
10. Added AssessmentLocationChangedNotification to OA\_Server.
11. Added GetActiveAssessmentLocations to INSP\_Server.
12. Deleted AssessmentChangedNotification from OA\_Server.
13. Delete GetCircuitElementsNearLatLong from INSP\_Server.
14. Addded GetOutageReasonCodes, OutageReasonContainerChangedNotification, and OutageReasonChangedNotification to OA\_Server.
15. Added the following calling parameters to the existing RestoreOutage method:

callbackCustomersThatCalled (bool), outageReasonContainer, and dispatcherResponsible (string).

1. Added dispatcherResponsible (string) to the existing SetOutageElementStatus method.
2. Changed CDStateChangedNotification to carry a CDStateChange object instead of a meterID and stateChange parameters.
3. Added an errorString parameter to the following methods that do not carry an object that inherits from an mspObject:
   1. PointSubscriptionListNotification
   2. FormattedBlockNotification
   3. IntervalDataNotification
   4. ReadingScheduleResultNotification
   5. AVLChangedNotification
   6. NumberCreatedNotification
4. Added InitiateLoadManagementEvent, InitiateLoadManagementEvents, InitiatePowerFactorManagementEvent, InsertInHomeDisplayInIHDGroup and RemoveInHomeDisplayFromIHDGroup on MDM\_Server.
5. Added OutageEventChangedNotification method to OD\_Server and MDM\_Server.
6. Changed EnableReadingSchedule to be EnableReadingSchedules in MDM\_Server and MR\_Server.

**Version 4.1 Release – Issued 06/30/2010.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**UML and Schema Changes:**

1. Changed namespace for this release to be: <http://www.multispeak.org/Version_4.1_Release>.
2. Added utility element to objectRef. This change applies both to the MultiSpeak UML model and the mspCPSM schema.
3. Added mspAlarm, blinkAlarm, and voltageAlarm.
4. Added the following elements to the content object: fileName, sourceFilePath, attachDateTime, and caption.
5. Revised identifiedObject fields in the mspObject to match the proposed CIM naming object. This change applies both to the MultiSpeak UML model and the mspCPSM schema.

**Web Service Method Changes:**

1. Changed the namespace for all web services to be: <http://www.multispeak.org/Version_4.1_Release>.
2. Added BlinkAlarmNotification and VoltageAlarmNotification to the OA\_Server, MDM\_Server, and NOT\_Server.
3. Added the following parameters to the AddAttachmentToWorkOrder method: workOrderID and objectRef.
4. Revised description of DeleteAttachmentFromWorkOrder to note that the binary content of an attachment (attachment.content) should not be included in the returned array of attachments.
5. Add the following methods to the DGN\_Server: GetAttachmentList and GetAttachment.
6. Add the following methods to the AM\_Server and GIS\_Server: GetAttachmentList, GetAttachment, AddAttachmentToWorkOrder, and DeleteAttachmentFromWorkOrder.
7. Add the following methods to the NOT\_Server: AddAttachmentToWorkOrder, and DeleteAttachmentFrom WorkOrder.
8. Changed the capitalization of “ID” to match the convention in the following methods:
   * CB\_Server.GetMeterByMeterID
   * CB\_Server.GetCustomerByCustomerID
   * CB\_Server.GetServiceLocationByCustomerID
   * CB\_Server.GetMeterBaseByObjectID
   * MDM\_Server.GetMeterBaseByObjectID
   * GIS\_Server.GetTransformerBankByUnitID

**Version 4.1 Release Candidate e – Issued 06/11/2010.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**UML and Schema Changes:**

Added notation in the web services message header schema that the Version attribute must contain the version number, release candidate and/or build information in the format shown in the message schema used for data included in the message to which this header is attached.

1. Changed namespace for this release to be: http://www.multispeak.org/Version\_4.1\_RC\_e
2. Corrected the multiplicity on worker.skillslist.skillID to be (0-\*) rather than (0-1).
3. Renamed mspDeviceHistoryEvent to be mspAssetHistoryEvent.
4. Added mspAssetHistoryEvent.informationList.
5. Added assetHistoryEvent.
6. Refactored intervalData.
7. Changed electricNameplate.multiplier to be of type float instead of type long.
8. Refactored accountsReceivable. Made acRecvBal, acRecvCur, acRecv30, acRecv60, and acRecv90 inherit from a new acctsReceivable class and added acRecvOtherList and acRecvItem to accommodate other types of accounts receivable.
9. Changed meterStatus to have a soft enumeration rather than a hard enumeration list.
10. Deleted meterReading.serviceType since serviceTye is already a part of meterReading.meterID.
11. Renamed connectDisconnectEvent.reasonCode to be connectDisconnectEvent.CDReasonCode.
12. Added PPMBalanceNegative, PPMBalancePositive, Other and Unknown to the enumeration for CDReasonCode.
13. Change name of intervalDataStatusCode, intervalDataStatusCodeEntry, and IntervalDataStatusCodeList to be readingStatusCode, readingStatusCodeEntry, and readingStatusCodeList.
14. Refactored readingStatusCode to match IEC 61968-9, Annex D QualityCodes.
15. Added meterReading.eadingValues.readingStatusCode.
16. Removed virtualMeter from model since it is not ready for release. It will be added back in the V4.2.1 prerelease build.
17. Added outageEventStatus.outageAttachments to carry either Text-to-Speech message transcriptions or pointers to voice recordings describing outageEvent status.
18. Added meterID.utility and the annotation to suggest that the contents of the meterID be the string concatenation of the utility, serviceType and objectID attributes separated by periods as follows: <utility>.<serviceType>.<objectID> .
19. Added “D-Y one” to enumeration list for wdgCode.
20. Changed the name of readingTypeID to be readingTypeCode to avoid confusion with the objectID of a readingType object.
21. Added readingTypeCode to a readingValue.
22. Added “any” attribute to readingStatusCode and meterEvent for extensibility and flexibility to adopt changes issued in these elements by future versions of IEC 61968-9.
23. Added domainNameChange and domainMember.action to facilitate publishing changes to domain information.

**Web Service Method Changes:**

1. Changed the namespace for all web services to be: "http://www.multispeak.org/Version\_4.1\_RC\_e"
2. Made all Initiate-type, Modify-type, or Notification-type services return an optional array of errorObjects.
3. Added DomainNamesChangedNotification and Domain MembersChangedNotification to all servers.
4. Added the following methods to the AM\_Server:

|  |
| --- |
|  |
| * CDDeviceAddNotification |
| * CDDeviceChangedNotification |
| * CDDeviceExchangeNotification |
| * CDDeviceInstalledNotification |
| * CDDeviceRemoveNotification |
| * CDDeviceRetireNotification |
| * EndDeviceShipmentNotification |
| * GetMeterTestByMeterID |
| * InHomeDisplayAddNotification |
| * InHomeDisplayChangedNotification |
| * InHomeDisplayExchangeNotification |
| * InHomeDisplayInstalledNotification |
| * InHomeDisplayRemoveNotification |
| * InHomeDisplayRetireNotification |
| * InspectionNotification |
| * LMDeviceAddNotification |
| * LMDeviceChangedNotification |
| * LMDeviceExchangeNotification |
| * LMDeviceInstalledNotification |
| * LMDeviceRemoveNotification |
| * LMDeviceRetireNotification |
| * MeterAddNotification |
| * MeterBaseAddNotification |
| * MeterBaseChangedNotification |
| * MeterBaseExchangedNotification |
| * MeterBaseInstalledNotification |
| * MeterBaseRemoveNotification |
| * MeterBaseRetireNotification |
| * MeterChangedNotification |
| * MeterEventNotification |
| * MeterExchangeNotification |
| * MeterInstalledNotification |
| * MeterRemoveNotification |
| * MeterRetireNotification |
| * MeterTestNotification |
| * ODDeviceChangedNotification |
| * PMChangedNotification |
| * PoleChangedNotification |
| * PPMMeterExchangeNotification |
| * SecurityLightChangedNotification |
| * ServiceOrderOpenedNotification * ServiceOrderChangedNotification * ServiceOrderClosedNotification * StreetLightChangedNotification |
| * TrafficLightChangedNotification |
| * TransformerBankChangedNotification * WorkOrderNotificationToGIS |

1. Added the following methods to the NOT\_Server:
   1. InspectionNotification
   2. MeterTestNotification

* ServiceOrderOpenedNotification
* ServiceOrderChangedNotification
* ServiceOrderClosedNotification

1. Deleted LoadManagementDeviceChangedNotification from the GIS\_Server and NOT\_Server.
2. Added the following methods to the GIS\_Server, FA\_Server, and DGN\_Server:
   1. AddAttachmentToWorkOrder
   2. DeleteAttachmentFromWorkOrder
3. Added the following methods to the CB\_Server:
   1. GetServiceOrdersByStatus
   2. GetServiceOrdersByServiceLocation
   3. GetServiceOrderByServiceOrderID
4. Removed the following methods from CB\_Server and MDM\_Server:
   1. GetMeterByMeterNo
5. Added the following methods to the DGN\_Server, MR\_Server, and MDM\_Server:
   1. ServiceOrderOpenedNotification
   2. ServiceOrderChangedNotification
   3. ServiceOrderClosedNotification
6. Added IntervalDataNotification to EA\_Server.
7. Added lastReceived to the following methods on MR\_Server and MDM\_Serverthat return a formattedBlock so that these methods can be sent in manageable blocks:

* GetLatestMeterReadingsByMeterGroups
* GetLatestReadingsByMeterIDAndFieldName

1. Added the following methods to return metered data in intervalData blocks in addition to the existing formattedBlocks:

* GetReadingsByBillingCycleIntervalData
* GetReadingsByMeterIDIntervalData
* GetReadingsByDateIntervalData
* GetLatestMeterReadingsByMeterGroupIntervalData
* GetLatestReadingsByMeterIDAndFieldNameIntervalData
* GetLatestReadingsByFieldNameIntervalData
* GetReadingsByDateAndFieldNameIntervalData
* GetReadingsByMeterIDAndFieldNameIntervalData
* GetLatestReadingsByMeterListIntervalData

1. Change name of GetIntervalDataStatusCodes to be GetSupportedReadingStatusCodes on MR\_Server and MDM\_Server.
2. Changed name of MeterTestTransaction to be MeterTestNotification to match our naming convention and fixed the method to carry an array of testedElectricMeter rather than meterTest. Changed on CB\_Server, MR\_Server, and MDM\_Server.
3. Added MeterTestNotification to NOT\_Server.
4. Changed the name of the InitiateMeterReadsByFieldName to be InitiateMeterReadingsByFieldName and modified annotation to reflect that data could be returned in ReadingChangedNotification, IntervalDataNotification or FormattedBlockNotifcation. Changes made on MR\_Server and MDM\_Server.
5. The following methods were renamed on the MR\_Server and MDM\_Server:

|  |  |
| --- | --- |
| Name in V4.1 RC d | Name in V4.1 RC e |
| GetLatestReadingByMeterNoAndType | GetLatestReadingByMeterIDAndFieldName |
| GetReadingsByDateAndType | GetReadingsByDateAndFieldName |
| GetReadingsByMeterNoAndType | GetReadingsByMeterIDAndFieldName |
| InitiateMeterReadByMeterNoAndType | InitiateMeterReadingByMeterIDAndFieldName |
| GetLatestReadingByType | GetLatestReadingByFieldName |
| InitiateMeterReadByMeterNumber | InitiateMeterReadByMeterID |
| InitiateGroupMeterRead | InitiateGroupMeterReading |
| ScheduleGroupMeterRead | ScheduleGroupMeterReading |
| InitiateMeterReadByObject | InitiateMeterReadingByObject |
| InitiateLPMeterReadByMeterNumber | Deleted |
| InitiateLPMeterReadsByMeterID | InitiateLPMeterReadingsByMeterID |
| InitiateMeterReadsByFieldName | InitiateMeterReadingsByFieldName |
|  |  |

1. The following methods were renamed on the CB\_Server:

|  |  |
| --- | --- |
| Name in V4.1 RC d | Name in V4.1 RC e |
| GetAccountByMeterNumberAndServiceType | GetAccountByMeterIDAndServiceType |
| GetServiceLocationByMeterNo | GetServiceLocationByMeterID |
| GetMeterByMeterNo | Deleted |
| GetMeterGroupNamesByMeterNo | GetMeterGroupNamesByMeterID |
| GetUsageByMeterNo | GetUsageByMeterID |
| GetCustomerByMeterNumberAndServiceType | GetCustomerByMeterIDAndServiceType |
|  |  |

1. The following methods were renamed on the DR\_Server:

|  |  |
| --- | --- |
| Name in V4.1 RC d | Name in V4.1 RC e |
| GetLoadManagementDeviceByMeterNumber | GetLoadManagementDeviceByMeterID |
|  |  |

1. The following methods were renamed on the EA\_Server:

|  |  |
| --- | --- |
| Name in V4.1 RC d | Name in V4.1 RC e |
| GetMeterConnectivityByMeterNo | GetMeterConnectivityByMeterID |
|  |  |

1. The following methods were renamed on the OD\_Server:

|  |  |
| --- | --- |
| Name in V4.1 RC d | Name in V4.1 RC e |
| GetOutageDetectionDevicesByMeterNo | GetOutageDetectionDevicesByMeterID |
|  |  |

**Version 4.1 Release Candidate d – Issued 03/30/2010.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**Schema Changes:**

**Added notation in the web services message header schema that the Version attribute must contain the version number, release candidate and/or build information in the format shown in the message schema used for data included in the message to which this header is attached.**

1. Added statuses to meterStatus enumeration.
2. Added meterStatusList to mspMeter.
3. Added meterBaseExchange object.
4. Added acRecv30DateDue, acRecv60DateDue, acRecv90DateDue elements to account.accountsReceivable.
5. Deleted meterRead.
6. Added virtualMeter class.
7. Added formattedBlockTemplate
8. Added expirationTime and sampleRate simpleTypes.
9. Added fieldName to meterReading.readingValues.readingValue. Deleted meterReading.readingValues.readingValue.readingValueType and meterReading.readingValues.readingValue.otherReadingValueType.
10. Renamed tender.transactionID to be tender.financialTransactionID to avoid confusion with the transactionID in the method parameter list.
11. Added electricMeter.meterBaseID..
12. Added annotation in the UML model and schema to indicate that the any in the MultiSpeak container object should be restricted to contain objects that inherit directly or indirectly from the mspObject..
13. Added actions to actionTaken enumeration.
14. Added mspDeviceHistoryEvent.
15. Added MeterHistoryEvent of type mspDeviceHistoryEvent.
16. Changed MeterConnectivity.oldFeeder to be oldFeederName, MeterConnectivity.newFeeder to be newFeederName, MeterConnectivity.oldFeederNo to be oldFeederNumber, MeterConnectivity.newFeederNo to be newFeederCode for consistency.
17. Changed electricMeter.electricLocationFields.feeder to be feederCode for consistency and fixed annotation.
18. Added intervalDataStatusCodeList class.
19. Changed attachment to inherit from mspObject so instances can be acted on.

**Web Service Method Changes:**

1. Added the following methods to the SCADA\_Server and DA\_Server:
   1. GetSCADAAnalogsByDateRangeAndPointID
   2. GetSCADAStatusesByDateRangeAndPointID
   3. GetSCADAStatusesByDateRange
   4. GetSCADAAnalogsByDateRangeAndPointIDFormattedBlock
   5. GetSCADAStatusesByDateRangeAndPointIDFormattedBlock
   6. GetSCADAStatusesByDateRangeFormattedBlock
2. Added GetMeterBaseByObjectID to the MDM\_Server and CB\_Server.
3. Added the following methods to the CB\_Server, MDM\_Server, and NOT\_Server:
   1. MeterBaseExchangeNotification
   2. MeterBaseInstalledNotification
4. Added the following methods to the MR\_Server, MDM\_Server, and NOT\_Server:
   1. MeterBaseAddNotification
   2. MeterBaseChangedNotification
   3. MeterBaseExchangeNotification
   4. MeterBaseRemoveNotification
   5. MeterBaseRetireNotification
5. Added the following methods to the MR\_Server and MDM\_Server:
   1. InitiateMeterReadsByFieldName
6. Added the following methods to the MR\_Server and MDM\_Server:
   1. GetFormattedBlockTemplates
   2. GetLatestReadingsByMeterListFormattedBlock
7. Documented in the MDM\_Server interface chart that an MDM application can have SCADA analogs, statuses and accumulator changes published to it by implementing a DA\_Server endpoint.
8. Add InitiateODEventRequestByServiceLocation to the MDM\_Server. This method was inadvertently omitted previously.
9. Add the MeterConnectivityNotification method that is currently in MR\_Server to the CB\_Server.
10. Add an optional expirationTime parameter to the end of the calling parameter list for the following methods:
    1. In DA\_Server and SCADA\_Server:
       1. InitiateStatusReadByPointID and InitiateAnalogReadbyPointID.
    2. In CD\_Server and MDM\_Server:
       1. InitiateArmCDDevice
       2. InitiateCDStateRequest
       3. InitiateConnectDisconnect
       4. InitiateDisableCDDevice
       5. InitiateEnableCDDevice
    3. In OD\_Server and MDM\_Server:
       1. InitiateODEventRequestByObject
       2. InitiateODEventRequestByServiceLocation
       3. InitiateODMonitoringRequestByObject
       4. InitiateOutageDetectionEventRequest
    4. In MR\_Server and MDM\_Server
       1. InitiateDemandReset
       2. InitateGroupMeterRead
       3. InitateMeterReadByMeterNoAndType
       4. InitatiateMeterReadByMeterNumber
       5. InitatiateMeterReadByObject
11. Remove readingType and add optional formattedBlockTemplateName and array of fieldname to the following methods in MR\_Server and MDM\_Server:
    1. GetReadingsByBillingCycle
    2. GetReadingByMeterNumberFormattedBlock
    3. GetReadingsByDateFormattedBlock
    4. GetLatestMeterReadingsByMeterGroup
    5. GetLatestReadingsByMeterNoAndType
    6. GetLatestReadingsByType
    7. GetReadingsByDateAndType
    8. GetReadingsByMeterNoAndType
    9. GetLatestReadingsByMeterNoList
12. Added GetAllConnectDisconnectEventsByReasonCode to CB\_Server and MDM\_Server.
13. Added ConnectDisconnectChangedNotification to MDM\_Server.
14. Added ModifyWorkOrderStatusByObjectID to DGN\_Server.
15. Added GetMeterHistoryByMeterID to CB\_Server..
16. Replaced GetSupportedReadingTypes with GetSupportedFieldNames in MR\_Server and MDM\_Server.
17. Replaced readingType with fieldname in calling parameter list for the following methods in MR\_Server and MDM\_Server:
    1. InitiateMeterReadByMeterNoAndType
18. Added GetIntervalDataStatusCodes to MR\_Server and MDM\_Server.

**Version 4.1 Release Candidate c – Issued 11/30/2009.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**Schema Changes:**

1. Fixed objectRef to inherit from xs:string by extension.
2. Fixed shortCircuitAnalysisResult.faultImpedance to be of type complexImpedance rather than impedance.
3. Added definition of gpsPoint.
4. Rolled back the addition of the GPS element to mspPointObject that was made in V4.1, release candidate b and added two new optional elements: gpsPoint and gpsLocation.
5. Added a new element, callBackListType, to the callBackList.
6. Made latitude and longitude mandatory in the gpsLocation object.
7. Added a new accumulatedValue object to act as a SCADA accumulator and added “accumulator” to the simpleType scadaPointType.
8. Added new content, attachment, and attachments objects to carry binary content files.
9. Replaced assessment.photo with assessment.attachments.
10. Added attachments to assessmentLocation.
11. Deleted message.wavPointer and added attachments and transcription to message.
12. Added attachments to station and design objects and removed contentReferences from station and design.
13. Deleted inspectionDataSet, inspectionSetDraft and added inspection.
14. Removed assetFields from transformerBank, since transformerBanks are not assets. The assetFields should properly only be on the transformer instances which are assets. Similarly, assetFields were added to capacitors, regulators, secondaryJunctionBoxes, primaryCabinets, inHomeDIsplays, loadManagementDevice, outageDetectionDevices, measurementDevices, meterBases, streetlights, securityLights, trafficLights and power systemDevices, along with objects that inherit from the mspDevice and mspSwitchingDevice.
15. Removed maxLength attributes from firstName and middleName. These should have been removed during the transition to V4, but were overlooked.
16. The usageInstance.rate is now the new rate object rather than merely a string field.
17. Added description element to serviceLocation.
18. Made the UTCOffset attribute mandatory on the timeZone object.
19. Added rateCode to rate object.
20. Specified that meterEvent.type and meterEvent.value should be of type string; previously they were undefined.
21. Deleted diagnosisDataSet and added observation.
22. Changed the element assessment.created to be assessment.closedOn.
23. Reordered assessment.closedOn and assessment.closedBy.
24. Added assessment.elementID.
25. Added extensions and extensionsList to the switchingDevice choice and to the overCurrentDevice choice.
26. Added gpsPoint to mspMeter.utilityInfo.
27. Changed the name of mspMeter.utilityInfo.mapLocation to be mspMeter.utilityInfo.GMLLocation to match V4 practice.
28. Changed the name of billingAccountLoad.mapLocation to be billingAccountLoad.GMLLocation to match V4 practice.
29. Replaced the inspection.GMLLocation with an inspection.geometry so that the inspection could exhibit polygon or line geometry if appropriate.
30. Renamed waterMeter.waterLocationFields.**gas**ServiceID to be waterMeter.waterLocationFields.**water**ServiceID.
31. Renamed waterMeter.waterlocationFields.**msp**extensionsList to be waterMeter.waterlocationFields.extensionsList.
32. Added readingTypeID to readingValue.
33. Added impedances object to eliminate anonymous type on capacitorBank object.
34. Added “Service drop” to list of enumerated values for the equipmentType simple type.
35. Changed the “ratedAmps” element on the recloserEntry to be “ratedCurrent” to match established usage.
36. Added extensions, extensionsList, and inHomeDisplayList elements to meterBase.deviceList.
37. Added missing extensions element definition.
38. Added “Other” and “Unknown” as enumerations in powerMonitor, measurementDeviceStatus and outageDetectDeviceStatus.
39. Added “Unknown” to outageDetectDeviceType enumeration list.
40. Fixed spelling of initialReactiveCapabilityCurve on synchronousMachine.
41. Added cut, jumper, and elbow to physicalObjectList.
42. Removed length restriction on electrican and contractor simple types.
43. Added taskListItem and changed taskList to be a list of taskListItem.
44. Changed name of taskListItem.workTask to be taskListItem.workTaskID to match convention.
45. Declared taskAggregation.workTaskID to be of type objectID.
46. Changed billingAccountLoad.serviceType to be billingAccountLoad.servType, to reflect the fact that this is intended to be a rate code not a utility type (serviceType).
47. Added “Opened” and “Close” to the enumeration list loadActionCode.
48. Made ppmBalanceAdjustment.serviceType to be of type serviceType rather than xs:string.
49. Corrected spelling of switchingDeviceBank in enumeration list of circuitElement.elementType.
50. Added electricService, streetlight, securityLight, and trafficLight to and deleted serviceLocation and substation from enumeration list of circuitElement.elementType.
51. Fixed spelling of contentReference.
52. Fixed customersAttachedToDevice.deviceID to be of type objectRef.
53. Fixed spelling of contactInfo.otherContactInformation.
54. Added “Kilometers” to enumeration list for materialItems.
55. Renamed resource.workerList to be resource.workers to avoid confusion with workerList that inherits from crewMemberList.
56. Fixed inHomeDisplayBillingMessage.usedLastMonth, inHomeDisplayBillingMessage.usedFourWeeksAgo, and inHomeDisplayBillingMessage.usedThisMonthLastYear to be of type money rather than commodityUsage.
57. Eliminated simpleType “value” and replaced with simple type”valueFloat” of type float. Added complex type “value” of type float with attribute “units” of type “uom”.
58. Added back in electricMeter.sealNumberList, which was inadvertently dropped in the transition to V4.0.0.
59. Deleted empty and unused “specifiedDate complexType.
60. Changed workTicket.wrhsCode to be workTicket.warehouseID to match workOrder practice.
61. Changed workTicket.crewCode to be workTicket.crewID to match workOrder practice.
62. Corrected case on overcurrentDevice and overcurrentDeviceList.
63. Added transactionID to tender.
64. Added callerID to outageCustomer.
65. Added cpsm:TimeSpan and made cpsm:Accumultor.timeSpan to be of type TimeSpan to eliminate anonymous element definition.

***Changes that have been made in UML-generated version of the V4.1 schema:***

1. Added guyList to pole to implement a guy-pole association, previously missing in MultiSpeak.
2. Added optional list of accounts, workList, workOrderList, maintenanceOrderList, and serviceOrderList to customer object.
3. Added optional list of serviceLocations, workList, workOrderList, maintenanceOrderList, and serviceOrderList to account.
4. Added an optional workList, workOrderList, maintenanceOrderList, and serviceOrderList to serviceLocation.
5. Added optional electricMeter and inHomeDisplays (list object) to the meterBase.
6. Added an optional meterBase object on the electricService.
7. Added an optional waterMeter on a waterService.
8. Added an optional gasMeter on a gasService.
9. Added optional otherMeter to otherService.
10. Added optional serviceOrderList, maintenanceOrderList, jobList, outageTicketList, workList and workOrderList to project.
11. Added optional premiseObjectList to parcel.
12. Added optional serviceLocations to premise.
13. Ordered uom enumeration alphabetically.
14. Ordered physicalObjectList and CIMObjectList alphabetically.
15. Changed workOrder.contentReference to be workOrder.attachments.
16. Added workers, crewEquipmentList, vehicles, and capabilities to crew.
17. Added workers, crews, vehicles, and crewEquimentlist to resource.
18. Added tasks on work object.
19. Added outageEventStatus and outageCustomerList to outageEvent object to build associations.
20. Added optional profile object to intervalBlock.
21. Added optional switchingScheduleList and switchingSteps to work and resource objects.
22. Added optional crewActionEvents list on the outageEvent object.
23. Added inHomeDisplays to inHomeDisplayGroup.
24. Added inHomeDisplayBillingMessageList and inHomeDisplayMessageList to inHomeDisplay object.
25. Changed measurementItems.accumulator to be of the new accumultatedValue type instead of cpsm:Accumulator.

**Web Service Method Changes:**

1. Added AccumulatedValueChangedNotification to SCADA\_Server, DA\_Server, and NOT\_Server.
2. Added to MR\_Server, and rolled back addition to CB \_Server made in V4.1 RC b:
3. GetConfigurationGroupNames
4. GetConfigurationGroupMembers
5. GetConfigurationGroupNamesByMeterNo

**Version 4.1 Release Candidate b – Issued 08/26/2009.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**Schema Changes:**

1. Added RegistrationID to the MultiSpeak web services message header (MultiSpeakMsgHeader).
2. Added registrationInfo object.
3. Added switchingOrder, switchingSchedule, switchingStep, and clearance objects.
4. Fixed spelling of GMLPolygons object.
5. Added CDState object.
6. Added timeZone object and added timeZone on mspPointObject. Note that this is a breaking change from V4.0.0, but the group agreed to adopt this breaking change.
7. Added GPS element to mspPointObject and thus, to every object that inherits directly or indirectly from the mspPointObject. Note that this is a breaking change from V4.0.0, but the group agreed to adopt this breaking change- **Rolled back 09/29/2009. Added modified mapLocation.**
8. Added assessment, assessmentList, assessmentLocation, GPSLocationAndTolerance, and CircuitElementAndDistance objects.
9. Changed the streetlight and securityLight to inherit from the mspElectricPoint rather than the mspPointObject. Note that this is a breaking change from V4.0.0, but the group agreed to adopt this breaking change.
10. Added a new trafficLight object that inherits from the mspElectricPoint.
11. Change the outageEvent to inherit from the mspPointObject rather than an mspObject
12. Added meterEvent to CDStateChange.
13. Added the following actions to the loadActionCode: Arm, Enable, Disable.
14. Added the following states to the loadActionCode: Armed, Enabled, and Disabled.
15. Added the following states to the RCDState: Enabled and Disabled.
16. Added MessageID, TimeStamp, and Context to the MultiSpeak web services message header.
17. Added schedule, readingSchedule, readingScheduleResult, periodicSchedule, absoluteSchedule, timePoint, cimTimePoints, meterGroupList, configurationGroup, and configurationGroupList objects.
18. Added inHomeDisplayMessage, inHomeDisplayBillingMessage, inHomeDisplayGroup, and inHomeDisplayList objects.
19. Added rate, rateInfo, commodityUsage, usageOtherPeriod, and usageOtherPeriodList.
20. Added eventInstance, eventInstances and meterEventList.
21. Added outageEvent.outagedPhase.

**Web Service Method Changes:**

1. Added the following new functions:
   1. Switching Orders (SWO).
   2. Asset Management (AM)
   3. Inspection (INSP)
   4. Notification (NOT)
   5. HAN Communications (HAN)
2. Added the following optional methods to all functions:
   1. RequestRegistrationID
   2. RegisterForService
   3. UnregisterForService
   4. GetRegistrationInfoByID
   5. GetPublishMethods
3. Added a note in the description of every unsolicited notification-type message that the registrationID should be added in the message header to indicate to the subscriber under which registrationID they received this notification data.
4. Added the following methods to the SCADA\_Server:
   1. SCADAPointChangedNotification
   2. SCADAPointChangedNotificationForAnalog
   3. SCADAPointChangedNotificationForStatus
   4. SCADAAnalogChangedNotification
   5. SCADAAnalogChangedNotificationByPointID
   6. SCADAAnalogChangedNotificationForPower
   7. SCADAAnalogChangedNotificationForVoltage
   8. SCADAStatusChangedNotification
   9. SCADAStatusChangedNotificationByPointID
5. Added to CD\_Server and MDM\_Server. These methods are added to support harmonization with IEC 61968-9, Annex F.
   1. InitiateCDStateRequest
   2. InitiateArmCDDevice
   3. InitateEnableCDDevice
   4. InitateDisableCDDevice
6. Added to MR\_Server and MDM\_Server:
7. InitateDemandReset – This method is added to support harmonization with IEC 61968-9, Annex F.
8. InsertMetersInConfigurationGroup
9. RemoveMetersFromConfigurationGroup
10. Added to CB\_Server, MDM\_Server, and OA\_Server:
    1. CDStateNotification
    2. CDStatesNotification
11. Added to CB\_Server, and MDM\_Server: Sense is wrong, should be MR\_Server
12. GetConfigurationGroupNames
13. GetConfigurationGroupMembers
14. GetConfigurationGroupNamesByMeterNo
15. ReadingScheduleResultNotification
16. Added InitiateAVLUpdateRequest to AVL\_Server.
17. Added transactionID to AVLChangedNotification in GV\_Server, GIS\_Server, and SCHED\_Server.
18. Added the following methods to the CB\_Server:
    1. GetAllStreetLights
    2. ModifyCBDataForStreetLights
    3. GetAllSecurityLights
    4. ModifyCBDataForSecurityLights
19. Added the following methods to the GIS\_Server.
    1. StreetLightChangedNotification
    2. SecurityLightChangedNotification
    3. TrafficLightChangedNotification
20. Added the following methods to FA\_Server, and DGN\_Server:
21. GetAllLaborCategories
22. GetModifiedLaborCategories
23. LaborCategoryNotification
24. Added to MR server and MDM server:
    1. EstablishSchedules
    2. DeleteSchedule
    3. GetSchedules
    4. GetScheduleByID
    5. EstablishReadingSchedules
    6. EnableReadingSchedule
    7. DisableReadingSchedule
    8. DeleteReadingSchedule
    9. GetReadingSchedules
    10. GetReadingScheduleByID
    11. GetLatestReadingsByMeterNoList
25. Corrected the following methods to carry an array rather than a single instance in CB\_Server:
    1. ModifyCBDataForCustomer
    2. ModifyCBDataForServiceLocation
26. Added to INSP\_Server:
    1. AssessmentChangedNotification
    2. AssessmentLocationChangedNotification
    3. GetAssessmentLocations
    4. GetCircuitElementNearLatLong
    5. GetOutageByCircuitElement
27. Added to OA\_Server:
    1. ResolvedCaller
    2. UpdateMessageStatus
28. Added the following methods to the to the PPM\_Server and the HAN\_Server:
    1. InHomeDisplayMessageNotification
    2. InHomeDisplayBillingMessageNotification
    3. GetAllInHomeDisplays
    4. InsertInHomeDisplayInIHDGroup
    5. RemoveInHomeDisplayFromIHDGroup
    6. EstablishIHDGroup
    7. DeleteIHDGroup
29. Added the following methods to the HAN\_Server:
    1. InHomeDisplayAddNotification
    2. InHomeDisplayChangedNotification
    3. InHomeDisplayExchangeNotification
    4. InHomeDisplayRemoveNotification
    5. InHomeDisplayRetireNotification
30. Add in CB\_Server:
    1. GetIHDGroupNames
    2. GetIHDGroupMembers
    3. GetIHDGroupNamesByInHomeDisplayID
31. Added to SWO\_Server:
    1. GetSwitchingOrderByID
    2. GetSwitchingOrderByDateRange
32. Added to CB\_Server, WTG\_Server, EA\_Server, GIS\_Server, SCADA\_Server, OA\_Server, and NOT\_Server:
    1. SwitchingOrderChangedNotification
33. Added to CB\_Server, MDM\_Server, and NOT\_Server:
    1. MeterEventNotification
34. Added to OA\_Server:
    1. GetOutageByCircuitElement
35. Changed the description of the InitiateGroupMeterRead method on MR\_Server and MDM\_Server to reflect that this method schedules a reading from devices rather than returning the most recent read in the MR database.

**Version 4.0.1 Release Candidate a – Issued 04/14/2009.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**Schema Changes:**

1. Added switchingOrder, switchingSchedule and switchingStep objects.
2. Added CDState object.
3. Eliminated faulty xs:unique constraints for workOrderIdentifier, stationLocation, and stationID.

**Web Service Method Changes:**

None.

**Version 4.0.0 Release – Issued 02/01/2009.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**Schema Changes:**

1. Added elbow, jumper and cut objects.
2. Added elbow, jumper and cut as optional switchingDevices to the switchingDeviceBank.

**Web Service Method Changes:**

1. Made the following changes in the AVL\_Server:
   1. Changed the name of the GetAVLMessagesByVehicleAndDate to be GetAVLMessagesByAVLID for consistency with other naming conventions.
   2. Chang ed the name of the GetLastAVLPositionByVehicle to be GetLastAVLPositionByAVLID for consistency with other naming conventions
   3. Changed the name of the GetLatestAVLMessages to be GetLastAVLMessages for consistency with other naming conventions
   4. Added a new GetAVLMessagesByVehicleName for completeness.
2. Added the following methods to the OA\_Server:
   1. InitiateCut
   2. RestoreCut

**Version 4.0, Release Candidate d – Issued 1/22/2009.**

**General Comments:**

1. The Apache Axis web services toolkit has problems properly generating anonymous complex types. In this release candidate, all anonymous complex types were replaced by defined complex types.
2. In most cases, cardinality that was defined on an element was replaced with a list object that defines cardinality on the sequence for stylistic consistency. Exceptions are the MultiSpeak, CPSM, physicalObjectList and spatialFeatureGroup containers. In these cases the list objects would create significant, needless bloat.
3. In all cases the terms phase, phaseCode, and phases have been modified as necessary to have the following consistent meanings:
   1. **phase** is the single phase or neutral designation as defined using the mspPhase enumerated simpleType.
   2. **phases** is the number of phases included at that point in the system.
   3. **phaseCode** is the combination of phase and neutral designations defined using the phaseCode enumerated simpleType.
4. The meterID has been replaced with a complexType that has three attributes: meterNo, serviceType, and objectID. This is necessary to clearly establish which meter is bein indicated since there could be an electricMeter, and a gasMeter with the same objectID.
5. The serviceID has been replaced with a complexType that has two attributes, serviceType and objectID.
6. All value type objects have been rebuilt so that the units in the unit/value pair is carried in an attribute and the value is carried directly in the object, not as a sub-element in the object.
7. Added to the MultiSpeak message header schemas two new optional attributes: CoordinateSystemAuthority and CoordinateSystemAuthorityCode. These were added to support the addition of coordinate systems defined by coordinate system authorities, as described in the annotation to these new attributes.

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**Schema Changes:**

1. Fixed the gml namespace declaration in the multispeak.xsd schema.
2. Rolled back the change in nodeID that was made in release candidate c (Schema change #4).
3. Annotation was used to clearly identify any elements added simply to facilitate compliance with the CIM CPSM profile or to facilitate future CIM compatibility.
4. Added a new object geometry that includes multiple types of geometry. Used this new object in the definition of workLocation and the new abstract multi-geometry object (named mspMultiGeometryObject). Changed the station object to inherit from the mspMultieometryObject abstract class.
5. Added contentReferences to designs and stations on designs.
6. Added designIdentifier and workFlowStatus to design object.
7. Eliminated the use of different service locations for each service type (electric, gas, water, propane, etc). Instead added “services” structures to a single serviceLocation object to support multiple electricService, waterService, gasService, propaneService instances at a single serviceLocation.
8. Enumerated the serviceType simpleType using the following enumeration list: Electric, Gas, Water, Propane, Refuse, Sewer, Telecom, TV, Cable, Heating, Steam, Transportation, All, Other, Unknown.
9. Renamed the AVLEvent to be AVLState and modified content.
10. Renamed AVLLocation to be AVLLog and changed content.
11. Added AVLPosition object.
12. Replaced employee and crewmember objects with worker object.
13. Added a human-readable objectName element on the mspObject. This designator can be used to provide further information or identification where the objectID might be unknown or too terse. This can be used in a similar manner to facilityID or meterNo.
14. Adopted the Utilities Standards Board meter event codes structure.
15. In numerous locations:
16. Replaced the string “kW” in element names with “realPower”
17. Replaced “kV” with “voltage”
18. Replaced kVAr with “reactivePower”
19. Added complex types for real energy (kwh) and reactive energy (kVArh).
20. Moved the ssImedance, transImedance, and stImpedance from the inductionMachine to the synchronousMachine. Added replaced leakageReactance with magnetizingImpedance on inductionMachine and inductionMachineEntry.
21. Added “CenterTapSecondary” to the enumeration for the transformer winding code.
22. Added the historyComment object.
23. Added a thickness object and thicknessUnits.
24. Added ROWAttributes, inductionMachineEntry, and synchronousMachineEntry engineering catalog entries.
25. Moved fuse.linkRtg to fuseEntry.linkRtg. Added fuseSpeed to fuseEntry.
26. Removed condPerPhase from line definitions since it is now carried in the conductors child object.
27. Moved regulator.kVA to regulatorEntry and renamed ratedPower.
28. Added counts element to sectionalizer. Added maxCounts, isLoadBreak, and resetTime to sectionalizerEntry.
29. Changed transformer winding phase shift to be measured in “clock position” rather than degrees to match industry practice.
30. Removed the following unused simpleTypes: conductorPerPhase, mspPhaseA, mspPhaseB, and mspPhaseC.
31. Added enumeration list (Hot, Cold, Other, Unknown) to station.constType.
32. Added affectedRelay element to powerFactorManagementEvent.
33. Rolled back the deletion of groupName in the loadManagementEvent object.
34. Moved the backgroundGraphics object from the workOrder to the design object.
35. Fixed odometer to match unit/value convention.
36. Added taskAggregation object.

**Web Service Method Changes:**

1. Added the following methods to MR\_Server and MDM\_Server:
   1. GetLPReadingsByMeterIDIntervalData
   2. GetLPReadingsByDateIntervalData
   3. GetLPReadingsByBillingCycleIntervalData
   4. InitiateLPMeterReadsByMeterID
2. Added the following methods to the MDM\_Server:
   1. IntervalDataNotification
   2. GetElectricMetersByAccountNumber
   3. GetGasMetersByAccountNumber
   4. GetWaterMetersByAccountNumber
   5. GetPropaneMetersByAccountNumber
3. Added the following methods to the CB\_Server:
   1. IntervalDataNotification
   2. TaskListNotification
   3. WriteAccountHistoryComments
   4. GetProjects
   5. GetAllOtherMeters
   6. GetElectricMetersByAccountNumber
   7. GetGasMetersByAccountNumber
   8. GetWaterMetersByAccountNumber
   9. GetPropaneMetersByAccountNumber
4. Added the following methods to the DGN\_Server:
   1. ProjectChangedNotification
   2. GetFAProject
   3. GetTaskAggregation
5. Added the following method to the WTO\_Server:
   1. GetTaskAggregation
6. Added NumberCreatedNotification method to the WTG\_Server.
7. Added the following methods to the WTP\_Server:
   1. GroupAssignmentNotification
   2. UnassignmentNotification
8. Added the following methods to the FA\_Server:
   1. GetProjects
   2. UpdateProjects
9. Modified description on GetDomainNames on every server to reflect the suggested practice of returning domain names in the form of noun.fieldname where “noun” is a defined MultiSpeak noun and fieldname is a sub-element of “noun”.
10. Added the following methods to the AVL\_Server (within a date/time range):
    1. GetAVLPositionsByAVLID
    2. GetAVLPositionsByVehicleName
    3. GetLastAVLPositions (all vehicles)
    4. GetLastAVLPositionByVehicle
    5. GetAVLMessages (with parameter = #of messages to return, keep asking until all returned)
    6. GetLatestAVLMessages
    7. GetAVLMessagesByVehicleAndDate
11. Removed AVLNotification from OA\_Server.
12. Fixed the spelling of the following method names on the DR\_Server:
    1. InitiateLoadManagementEvent
    2. InitiateLoadManagementEvents
    3. InitiatePowerFactorManagementEvent
13. Modified the GetAVLLocation methods on the AVL\_Server to return AVLPosition objects. Also these methods were changed to return only positions within a date/time range.

**Version 4.0, Release Candidate c – Issued 11/17/08.**

**General Comments:**

1. This is the first release of MultiSpeak that has a complete implementation of the Common Power System Model (CPSM), an international standard profile for the exchange of transmission system model information that is based in the Common Information Model (CIM). The complete CIM data model and the subset of CIM that constitutes the CPSM are both maintained by the International Electrotechnical Commission (IEC) Technical Committee 57 (TC57) as parts of the IEC61970 series and the IEC61968 series of standards. Numerous changes have been made throughout the MultiSpeak connectivity model to facilitate support of CPSM and to permit additional harmonization efforts with other CIM profiles, as such are developed in the future. A new included schema, named mspCPSM.xsd, has been added to the MultiSpeak specification for this release. However, not all of the contents of that schema come from the CIM, since some MultiSpeak objects must be copied there in order to build a complementary set of CIM objects for use in the combined MultiSpeak implementation. Furthermore, it should be noted that changes have been made in the multispeak.xsd schema to support the CPSM implementation. Although this revision history document will outline the significant changes made to the MultiSpeak schema, the changes are too numerous and pervasive to document exhaustively. Users who are familiar with Version 3.0 of the MultiSpeak specification should use care in the use of MultiSpeak Version 4.0 to flag changes that may not be explicitly described herein.
2. This is the first release of MultiSpeak that has consistently and completely supported water, gas, and propane service types in addition to electric service on an equal basis. Meters, meter readings, meter exchanges, and service locations are associated with specific service types. Both schema objects and web service methods have been modified to make clear the service type(s) being handled. Users should take care and be aware that web service methods in the

http://www.multispeak.org/Version\_4.0

namespace may be named the same as a method that was previously published under the

http://www.multispeak.org/Version\_3.0

namespace, but may be changed to clearly identify the service types(s) to which they apply.

1. This is the first release of the MultiSpeak specification that supports international conventions for telephone numbers, addresses, currencies, and units of measures. Currencies are expressed using a currencyCode, as defined in the international standard ISO 4217, “Currency Names and Code Elements”. The new currencyCode simple type has an extensive list of currency codes as defined in ISO 4217. A new defaultCurrencyCode has been added to the MultiSpeak message header. If this value is set, then it is not necessary to add a currency code attribute in each element that carries currency values. If neither the currencyCode attribute, nor the defaultCurrencyCode are is set then the type of currency being referred to is indeterminate; it should not be assumed that monetary amounts are expressed in USD (United States dollars).
2. In previous releases of MultiSpeak, there was extensive use made of XSD substitutionGroups, both in defining the object hierarchy and in some cases (for instance, overCurrentDeviceBank and switchDeviceBank) in defining flexible choices within an object. Although these uses were acceptable within the W3C specification for XML Schemas, they created problems with certain software tools. Present best practice suggests that the only use of XSD substitutionGroups is to define container objects and that substitutionGroups not be nested (that is to say that they not be used to define object hierarchies of more than one layer in depth). In this release, choice selectors are used rather than substitutionGroups in object definitions. Furthermore, the only use of substitutionGroups is to ensure that (i) elements created from complex types that inherit from the mspObject, either directly or indirectly, are included in the MultiSpeak root container class and (ii) elements created from complex types that inherit from the mspCIMObject in the mspCPSM schema, either directly or indirectly, are included in the CPSM root container class. The CPSM root container class is then included in the MultiSpeak root container class so that the MultiSpeak class can contain an unbounded number of instances of all top level objects. This is in line with the current best practice recommendations.

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). Changes have been made in this release candidate to address the substitution group issues observed in earlier releases; it is believed that this has addressed all of the earlier substitution group issues. The only work-around for the cardinality issues that is known at this time is either to edit the affected objects directly or to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**Schema Changes:**

1. Throughout the schema, the use of xs:string, objectID and objectRef was standardized when used to refer to object identifiers. In all cases objectID was used to refer to an object where the name of the element or the context made it clear which MultiSpeak noun was being referred to. If it was unclear which MultiSpeak noun was being referred to then an objectRef was used. All pointers that were previously of type xs:string were replaced with the appropriate choice (objectID or objectRef) to match the previous rule. For instance, customerID always refers, both by context and by the name of the element, to a customer object; therefore the use of objectRef is not necessary. In the case of a parentSectionID (a pointer to a parent section of indeterminate noun type), it is unclear what type of noun is being referred to. In this case the use of an objectRef is appropriate so that the receiving system can tell which noun type and objectID for that noun type are being pointed to. Wherever xxxxID is used in MultiSpeak, it should be assumed that this element is a pointer to the xxxx object, either of objectID type or of type objectRef, as appropriate.
2. Added CIM IdentifiedObject (naming) fields as optional elements to the mspObject and all objects that inherit from it – effectively all top level objects in MultiSpeak. This will facilitate future harmonization between CIM and MultiSpeak.
3. Renamed mapLocation to be GMLLocation and complexLine to be GMLLine to clarify that they are Geography Markup Language objects and to match CIM use.
4. Changed all node identifiers from MultiSpeak style nodeIdentifier elements to a new object called NodeFields, which includes a nodeIdentifier, an optional pointer to a containing substation (which is required by the CPSM) and potentially pointers to measurements made at that node (which is also required by CPSM).
5. Renamed the V3.0 meterReading object, which was originally developed from the ANSI C12.19 meter reading object, to be meterReadingC1219 and deprecated its use in V4.0.
6. Added a new meterReading object that is appropriate for all service types. Eliminated mspMeterReading, electricMeterReading, waterMeterReading, gasMeterReading, propaneMeterReading, which were added in V4.0, rc b.
7. Added new elements to carry arrays of objects from all service types: meterExchanges, meters, serviceLocations.
8. Eliminated electric-specific fields from the utilityInfo object and added it to the mspMeter abstract class. The electric-specific fields were added back to the electricMeter in the electricLocationFields object. Similarly gasLocationFields, waterLocationFields and propaneLocationFields elements were added to the gasMeter, waterMeter, and propaneMeter respectively. Unless and until specific fields are defined for those objects, an extensionList was added to the gasLocationFields, propaneLocationFields, and waterLocationFields elements.
9. Added waterReceivedMeters, gasReceivedMeters, and propaneReceivedMeters as optional lists in the existing endDeviceShipment object and eliminated separate mspMeterShipment, waterMeterShipment, gasMeterShipment and propaneMeterShipment objects.
10. Added a new account object.
11. Reworked the mspServiceLocation to eliminate account-specific information and added it to the new account object. Revised layout of electricServiceLocation, gasServiceLocation, waterServiceLocation and propaneServiceLocation objects accordingly. Note that an account does not specify a service type, but it is linked to by serviceLocation(s) that specify service types. Thus, a single customer account could be used only for a single service type or for multiple service types as is the custom for a specific customer billing system. It is however assumed that accountNumber (the objectID of account objects) is unique across all service types.
12. The previously unused primary key designators were eliminated, for example:

<xsd:key name="loadManagementEventPK">

<xsd:selector xpath="loadManagementEvent"/>

<xsd:field xpath="@objectID"/>

</xsd:key>

1. Revised the spelling of numerous elements to match more modern conventions. For instance, in mspServiceLocation, budgBill became budgetBill, servStatus became serviceStatus, etc. Other affected fields and the affected objects include:

const => construction (mspElectricLine)

phaseCd => phaseCode (all locations)

operVolt => operatingVoltage (mspElectricLine and objects that inherit from it).

swType => switchType (capacitorBank)

swStatus=> switchStatus (capacitorBank)

connectionCd => connectionCode (capacitorBank)

swType => switchType (capacitorBank)

swOn => switchOn (capacitorBank)

swOff => switchOff (capacitorBank)

cntrCkt =>controlCircuit (capacitorBank)

1. The following elements were changed on the mspMotorGenerator:

ssDesc(of type string) => ssImpedanceID (pointer to new ZsmImpedanceEntry)

tranDesc(of type string) => tranImpedanceID (pointer to new ZsmImpedanceEntry)

stDesc(of type string) => stImpedanceID (pointer to new ZsmImpedanceEntry)

ratedkV => ratedVoltage.

1. The motor object was renamed inductionMachine and significantly changed to support CIM CPSM requirements and to generalize the motor model for either induction motors or induction generators.
2. The generator object was renamed synchronousMachine and significantly changed to support CIM CPSM requirements and to generalize the generator model for either synchronous motors or synchronous generators.
3. The NEMA type code was carried in an element named nemaTyp, of type long, which was a numeric code that referred to the string NEMA types. This was replaced with an element named nemaType, of type enumerated string, which contains the strings directly in an enumeration list.
4. In numerous cases an element that presumes the unit used to express it was replaced by an element named generally and a list of units. For instance ratedKV would be replaced with ratedVoltage, bankKvar would became bankRating, etc.
5. The previously named switchDeviceBank was renamed switchingDeviceBank for consistency, since a switchingDeviceBank is a bank of switchingDevice(s).
6. The name of the MultiSpeak date/time data type was changed from mspDate to mspDateTime to avoid confusion.
7. Added the crewName element to the crew object.
8. Made the association between vehicles, employees, and equipment with a crew be pointers rather than encapsulated objects.
9. Changed the name of the people associated with a crew to be crew members rather than employees, since members of a crew might not be employed by the utility. Added a new crewMember object that inherits from the mspPerson abstract class.
10. Removed mspVehicle abstract class and truck object. All vehicles are referred to as being vehicles rather than having both vehicles and trucks.
11. Made a feeder be a container class so that equipment could be encapsulated in a feeder if desired.
12. Associated an inHomeDisplay with a meterBase rather than a meter, since neither the meterBase nor the inHomeDisplay are unlikely to change location, while meters are more likely to be moved.
13. Added complexVoltage and complexImpedance objects.
14. Deleted the distributionSubstation object that was added in V4.0, rc a. Now any substation, regardless whether it is a transmission or distribution substation is modeled with the substation class.
15. Added the following objects:

VoltageMagnitude

voltageAngle

multiPartIdentifier

resource

workRequest

workStatus

assignment

work

workTask

project

design

maintenanceOrder

demandResponseEvent

substationLoadControlStatus

ZsmImpedanceEntry

meterGroups

catalogEntries

1. Added a pointer to an equipmentContainer to the mspElectricLine and mspElectricPoint fo compliance with CPSM. Note that in CIM EquipmentContainer can be both a concrete class and an abstract class from which other classes are inherited (such as substation, Bay, VoltageLevel, Line, etc), thus the pointer to an EquipmentContainer must be an objectRef, not an objectID.
2. Added the CPSM LoadCurve as an optional element on the loadSection.
3. Fixed kW and kVAr on the allocated object to match the new unit/value pair convention.
4. Added isRemotelyOperable element to mspSwitchingBank.
5. The simple type frequency was deleted and the complex type frequency was added to replace it, with a unit value pair.
6. Updated the spatialFeatureGroup and physicalObjectList containers to incorporate all appropriate items.
7. Added ohTransmissionLine and ugTransmissionLie objects.
8. Added “Substation” to the transformerBank.mounting enumeration list.
9. Added phaseTripRating to mspOverCurrentDeviceBank.
10. Revised the scadaAnalog to be compatible with the CIM Analog type measurement.
11. Added the following elements to the capacitorBank object in order to be compatible with CPSM:

reactiveRating

reactivePerSection

maximumSections

normalSections

regulatingControlID

impedances

1. Added a skill object to document the certified skills that a person can have, such as hot work, underground work, chain saw, traffic management, hazardous waste disposal, etc.
2. Added a capability object to describe the types of work that a crew is qualified to perform, such as hot work, tree trimming, etc.
3. Added inspectionDataSet, diagnosisDataSet and maintenanceDataSet to report on field inspection, failure diagnosis, and maintenance activities respectively.
4. Added mspMultiGeometryObject abstract type and made station be of type mspMultiGeometryObject.
5. Added “Transfer” and “Salvage” to unitActn.
6. Added transferMH and hotTransferMH to laborComponent. Added transferCost to laborCategory.
7. Added genericPolygonFeatureList to backgroundGraphics object.
8. Added “All” to the enumeration list for serviceType.
9. Added serviceType to the connectDisconnectEvent.

**Web Service Method Changes:**

1. Combined the following servers:
   * MR\_Server and LP\_Server =>MR\_Server
   * EDR\_Server and EDT\_Server => EDTR\_Server
   * DAD\_Server and DAC\_Server => DA\_Server
   * DGV\_Server and SGV\_Server => GV\_Server
2. Added the following servers:
   * AVL\_Server.
   * WTG\_Server
   * SCHED\_Server
   * WTO\_Server
   * WTP\_Server
   * WV\_Server
3. Renamed the following servers:
   * STK\_Server => DGN\_Server )Staking => Field Design)
   * LM\_Server =>DR\_Server (Laod Management => Demand Response)
4. All methods that refer to the meter object by objectID, meterNo, or meterID were rebuilt using the new meters object so that meters of all service types could be returned, unless the return type is explicitly of one service type. In addition, the serviceType parameter was added to all Get type methods requesting meter data so that meters could be requested by serviceType, unless there was already a specific method to get the meters by serviceType.
5. All methods that refer to the serviceLocation object were rebuilt using the new serviceLocations object so that service locations of all service types could be returned, unless the return type is explicitly of one service type. In addition, the serviceType parameter was added to all Get type methods requesting serviceLocations so that service locations could be requested by serviceType.
6. All methods that refer to the meterExchange object were rebuild using the new meterExchanges object so that meter exchanges of all service types could be returned, unless the return type is explicitly of one service type. In addition, the serviceType parameter was added to all Get type methods requesting meterExchange data so that meterExchanges could be requested by serviceType.
7. All objects that refer to the meterGroup object were rebuilt using the new meterGroups object so that meterGroups of all different service types and mixed service types could be sent.
8. Changed the input parameter of the GetEngineeringEquipment method on the EA\_Server to be of type equipmentType, which is an enumeration of the names of the types of engineering catalog entries. The returned object is a new object called catalogEntries.
9. Added a GetCatalogEntries method to the EA\_Server to return the defined engineering catalog entries. The calling parameter is an array of the catalogEntries returned by calling the GetElectricalEquipment method and the return parameter is a new container object called returnedCatalogEntries.
10. The following methods were added to the MR\_Server and MDM\_Server to exchange load profile information using formattedBlocks:
    * GetLPReadingByMeterNumberFormattedBlock
    * GetLPReadingsByDateFormattedBlock
    * GetLPReadingsByBillingCycle
    * InitiateLPMeterReadByMeterNumber
11. Added the following methods to support work management:
    * AssignmentNotification (DGN\_Server, WTP\_Server, CB\_Server)
    * InitiateWorkRequest (FA\_Server, CB\_Server, WTG\_Server)
    * NumberCreatedNotification (DGN\_Server, WTO\_Server)
    * InitiateTaskGeneration (WTG\_Server)
    * TaskListNotification (SCHED\_Server)
    * UpdateWorkStatus (SCHED\_Server)
    * UpdateOutageStatus (OA\_Server)
    * GetTaskStatus (SCHED\_Server)
12. Changed the name of StakedWorkOrderNotification to be DesignedWorkOrderNotification to complement the revised name of the design server.
13. Modified GetMeterByAMRType to request meters by AMRVendor and AMRDeviceType rather than the deprecated AMRType. Also made the reference to meter plural to reflect our convention.
14. Modified the GetMeterGroupMembers to return the new meterGroups object rather than an array of strings.
15. Added the following methods to the AVL\_Server:
    * GetAVLSupportedVehicles
    * GetAVLLocationByVehicleID
    * GetAVLLocationByVehicleName
16. Added AVLChangedNotification to the following servers:
    * GIS\_Server
    * GV\_Server
    * OA\_Server
    * SCHED\_Server
17. Added AccountChangedNotification to the following servers:
    * MR\_Server
    * CD\_Server
    * OA\_Server
    * CRM\_Server
    * GIS\_Server
    * GV\_Server
    * CH\_Server
    * MDM\_Server
18. Added the following methods to the CB\_Server and MDM\_Server:
    * GetAllAccounts
    * GetAccountByCustomerID
    * GetAccountByMeterNumberAndServiceType
    * GetAccountByServiceLocationAndServiceType

**Version 4.0, Release Candidate b – Issued 08/25/08.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. In addition, substitution groups are not created properly. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes and incorrect creation of some classes created using substitution groups (notably the MultiSpeak object). The only known work-around at this time is to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

**Schema Changes:**

1. Changed the namespace for XML data types to be xs: rather than xsd: to match common industry practice and IEC use.
2. Separated GML data objects into the gml: namespace.
3. Separated the CIM CPSM objects into the cpsm: namespace and removed them from the multispeak.xsd schema. Corrected object name capitalization to match CIM conventions and removed the “cim” prefix on objects imported from CIM.
4. Updated some of the CIM objects to match the CIM release named 61968MessagesSchemasRev09.zip, dated 10/1/2007. Complete harmonization will occur after IEC releases the final CIM V12 in late 2008.
5. Corrected the abstract attribute of all abstract complex types and elements.
6. Replaced the simple type poleUseCode with poleUse for consistency.
7. Added billingCycle to the utilityInfo element.
8. Added materialItemID to the pickList object.
9. Added optional detailed addressing fields to the proposed international address object.
10. Changed the currencyCode element on the money object to be an attribute.
11. Changed the units on all values and measurements to be attributes rather than elements.
12. Changed voltage ratings in overcurrent devices, generators, regulators, and transformers to match the voltages defined in the engineering equipment catalogs.
13. Added draft mspMeterReading, electricMeterReading, gasMeterReading and waterMeterReading objects.
14. Added requestedNumber structure that will be used to send work order, service order or other information.
15. Added strategy and scheduleDateTime to the loadManagementEvent.
16. Changed the base class for mspElectricLine/constr from xs:string to be msp:eaEquipID so that all pointers to engineering equipment catalogs are of type eaEquipID.
17. Added new object complexImpedance.
18. Added groundingImpedance element on mspBankObject, of type complexImpedance.

**Web Service Method Changes:**

1. Added new methods GetNextNumber and ReturnGeneratedNumber to the following web services:
   * CB\_Server
   * FA\_Server
   * OA\_Server
   * STK\_Server
2. Added GetWorkOrderSelectionByStatus and GetWorkOrderSelectionList to the FA\_Server web service.
3. Added InitiateLoadManagementEvents method to the LM\_Server web service to permit sending an array of loadManagementEvents.
4. Added GetMeterGroupNamesByMeterNo to MDM\_Server and CB\_Server web service.
5. Added GetMeterConnectivityByMeterNo, GetCircuitElementByObject, and GetConnectivityByObject to EA\_Server web service.
6. Added the following methods to the LM\_Server web service:
   * SCADAAnalogChangedNotification
   * SCADAAnalogChangedNotificationByPointID
   * SCADAAnalogChangedNotificationForPower
   * SCADAAnalogChangedNotificationForVoltage
   * SCADAStatusChangedNotification
   * SCADAStatusChangedNotificationByPointID
   * SCADAPointChangedNotification
   * SCADAPointChangedNotificationForStatus
   * SCADAPointChangedNotificationForAnalog

**Version 4.0, Release Candidate a  – Issued 05/15/08.**

**Known issues with this release:**

1) WDSLs included with this (and all previous releases) do not enforce all of the cardinality restrictions in the XML schemas included in the release. The use of the xsd.exe command line tool to generate C# classes from the core (multispeak.xsd) schema results in incorrect cardinality in some classes (notably the MultiSpeak object). The only known work-around at this time is to delete the complex and simple types listed in a WSDL and to import the multispeak.xsd XML schema into the WSDL. Further investigation of this issue is on-going.

Version 4.0, release candidate a was based on Version 3.0, build q with the changes described below.

1. ***Changes to Implement Internationalization and Foster Harmonization with IEC CIM***
2. Internationalized address format for all addresses. Added townCode to address.
3. Internationalized telephone number formats for all telephone numbers. Added new telephoneNumber complex type.
4. Changed all instances of money/currency to a new complex type, money, that includes an optional currency code, based on ISO 4217 currency codes. Added default currencyCode attribute to message header to eliminate the need to send the currencyCode element with every instance of money.
5. Changed all measurements and measured elements to be a complex type with a value and unit pair. This is done to internationalize the measurements, to more closely harmonize with the IEC CIM approach to measurements, and to add flexibility. The new elements include:
   * length
   * height
   * seconds
   * voltage
   * current
   * realPower
   * reactivePower
   * apparentPower
   * activePower
   * resistance
   * reactance
   * impedance
   * admittance
   * susceptance
   * conductance
   * capacitance
   * resistivity
   * temperature
   * pressure
   * percent
   * angle
   * exponent
   * PowerFactor
   * systemFrequency
   * tapStep
   * speed
   * odometer
   * powerLimitationValue
6. Changed phaseCd to be phaseCode with more complete list of possible phase combinations.
7. Added switchTimeDelay to capacitorBank.
8. Eliminated powerLimitationUnits from ConnectDisconnectEvent, since it is now in the revised powerLimitationValue complex type.
9. Added new abstract type mspPerson. Made customer and employee of type mspPerson. This more closely harmonizes with IEC CIM and makes use of new internationalized telephone numbers and address types.
10. Added capabilitiesList to crew object.
11. Added skillsList to employee.
12. Changed milesFromSource to be distanceFromSource in mspResultsBase for internationalization.
13. Eliminated customer-related fields and added in customer object in WorkOrder object. Changed all phone numbers to new internationalized format.
14. Added Mils, Yards, Millimeters, Decimeters, Centimeters, Meters, Kilometers, and Unknown to lengthUnits.
15. Added velocity units of measure to uom.
16. Added the following new objects to support transmission data exchanges using the IEC CPSM:
    * IEC61970Version
    * identifiedObject (nameFields)
    * geographicalRegion, subGeographicalRegion
    * hostControlArea, subControlArea
    * organization
    * basePower, baseVoltage, cimBasePower
    * equipmentContainer
    * connector, busbarSection, connectivityNode
    * transmissionSubstation
    * mspCIMObject, mspCIMConductingEquipment (abstract types)
    * regulatingCondEq
    * powerSystemResource
    * cimSwitch
    * recloseSequence
    * protectedSwitch
    * electricalProperties, switchProperties, breakerProperties
    * transmissionBreaker
    * disconnector
    * loadBreakSwitch
    * voltageLevel, bay
    * seriesCompensator, shuntCompensator, staticVarCompensator
    * curve, curveData, basicIntervalSchedule, regularIntervalSchedule, irregularIntervalSchedule, regulationSchedule, regularTimePoint, irregularTimePoint
    * powerTransformer, transformerWinding, terminal, tapChanger
    * cimLine
    * acLineSegment
    * nodeFields, toEndFields, fromEndFields
    * cimMeasurement, cimLimitSet, cimAnalog, cimAnalogLimit, cimAnalogLimitSet, cimDiscrete, cimAccumultor, cimStringMeasurement,cimAnalogValue, cimAccumultorValue, cimDiscreteValue, cimStringMeasurementValue, cimMeasurementValue, cimMeasurementType, cimMeasurementValueSource
    * energyConsumer, customerLoad, equivalentLoad, inductionMotorLoad, stationSupply, loadArea, areaLoadCurve, season, nonConformLoadCurve
    * synchronousMachine, generatingUnit, thermalGeneratingUnit, hydroGeneratingUnit,
17. ***Power System Model Changes.*** These changes implement (i) changes necessary to facilitate IEC Common Power System Model (CPSM) profile model exchanges, (ii) changes necessary to implement engineering equipment catalog exchanges, and (iii) changes recommended by T. E. McDermott in his IEEE articles, “Distribution System Data Exchanges to Support Line and Cable Parameter Calculations”, *Proceedings of the 2007 Power Engineering Society General Meeting*, Tampa, Florida, and “Open Source Data Translation for Distribution System and Transient Modeling”.
18. Added engineering line data catalogs for: conductors, conecentric neutral cables, tape shield cables, service cable, line construction, material attributes, line environment attributes, and right-of-way attributes.
19. Added engineering equipment catalogs for: transformers, regulators, breakers, fuses, reclosers, sectionalizers, switches, and load mixes.
20. Eliminated substation; replaced with distributionSubstation. Added mspSubstation and new transmissionSubstation. Made transmissionSubstation and distributionSubstation of type mspSubstation. Added nameFields and equipmentContainer objects to mspSubstation (and by reference to distributionSubstation) to more closely harmonize with IEC CIM.
21. Eliminated equivalent source information from distributionSubstation and added new equivalentSource object.
22. Replaced position in mspOverCurrentDevice with normalPosition. Added currentPosition element in mspOverCurrentDevice. Added interruptingRating in mspOverCurrentDevice.
23. Added groundTripEnabled and groundTripRating to recloser.
24. Added vOutV, fhHiV, reverseFlowR, and reverseFlowX to regulator. Changed units of ldcR and ldcX to be voltage on the regulator PT base rather than impedances.
25. Added enumerations for regType and wdgType on regulatorBank object.
26. Added “shuntUngroundedWye” as an option in the connectionCode simple type to describe capacitorBank connections.
27. Added horizontal and vertical coordinates, bundle spacing and number of conductors in a bundle to conductorList entries, and replaced condN entries with conductorList entries with phaseCode of “N”.
28. Changed type of billRef from xsd:long to xsd:string.
29. ***Other Changes***
30. Changed all instances of custID to customerID and servLoc to serviceLocationID to attempt to standardize objectID references to be nounID where “noun” is the MultiSpeak noun to which the ID refers.
31. Changed noOfCustomers in allocatedLoad from being of type float to being of type integer.
32. Removed meter; replaced with electricMeter. Eliminated serviceLocation; replaced with electricServiceLocation. Eliminated nameplate; replaced with electricNameplate. Replaced meterExchange with electricMeterExchange.
33. Added mspMeterShipment, gasMeterShipment, propaneMeterShipment, and waterMeterShipment.
34. Added received waterMeter, receivedGasMeter, and recievedPropaneMeter.
35. Removed the following simple types:
    * accountsReceivableBalance
    * addressLine
    * city
    * state
    * zip
    * custID
    * poleHeight